{"text_format":"1","workbook":"xlsx","n_sheets":28,"sheets":["B8","B9","B11","Atomic","ANTOINE","KOPPS","B3","Sheet1","Introduction","Chapter2","Chapter 3","Chapter 4","Chapter 5","Chapter 6","Chapter 7","Chapter 8","Chapter 9","Chapter 10","Chapter 11","B6","B5","B7","B7L","Steam Tables","Species","B1","B2","Solver"],"not_rendered":{"charts":0,"images":3,"macros":1,"external_links":0,"defined_names":61,"comments":9,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"B8","index":0,"n_rows":22,"n_cols":8,"rows_kept":22,"cut":false,"hidden":true,"merged":[]}
["Specific Enthalpies of Selected Gases: SI Units, Ĥ (kJ/mol)"]
[]
["Reference state: Gas, Pref = 1atm, Tref = 25°C"]
[]
["T","Air","O2","N2","H2","CO","CO2","H2O"]
[0,-0.72,-0.73,-0.73,-0.72,-0.73,-0.92,-0.84]
[25,0,0,0,0,0,0,0]
[100,2.19,2.2400000000000002,2.19,2.16,2.19,2.9,2.54]
[200,5.15,5.31,5.13,5.0599999999999996,5.16,7.08,6.01]
[300,8.17,8.4700000000000006,8.1199999999999992,7.96,8.17,11.58,9.57]
[400,11.24,11.72,11.15,10.89,11.25,16.350000000000001,13.23]
[500,14.37,15.03,14.24,13.83,14.38,21.34,17.010000000000002]
[600,17.55,18.41,17.39,16.809999999999999,17.57,26.53,20.91]
[700,20.8,21.86,20.59,19.809999999999999,20.82,31.88,24.92]
[800,24.1,25.35,23.86,22.85,24.13,37.36,29.05]
[900,27.46,28.89,27.19,25.93,27.49,42.94,33.32]
[1000,30.86,32.47,30.56,29.04,30.91,48.6,37.69]
[1100,34.31,36.07,33.99,32.19,34.369999999999997,54.33,42.18]
[1200,37.81,39.700000000000003,37.46,35.39,37.869999999999997,60.14,46.78]
[1300,41.34,43.38,40.97,38.619999999999997,41.4,65.98,51.47]
[1400,44.89,47.07,44.51,41.9,44.95,71.89,56.25]
[1500,48.45,50.77,48.06,45.22,48.51,77.84,61.09]

{"sheet":"B9","index":1,"n_rows":27,"n_cols":8,"rows_kept":27,"cut":false,"hidden":true,"merged":[]}
["Speicific Enthalpies of Selected Gases: American Engineering Units, Ĥ (Btu/lb-mole)"]
[]
["Reference state: Gas, Pref = 1atm, Tref = 77°F"]
[]
["T","Air","O2","N2","H2","CO","CO2","H2O"]
[32,-312,-315,-312,-310,-312,-394,-361]
[77,0,0,0,0,0,0,0]
[100,160,162,160,159,160,206,185]
[200,858,875,857,848,859,1132,996]
[300,1563,1602,1558,1539,1564,2108,1818]
[400,2275,2342,2265,2231,2276,3129,2652]
[500,2993,3094,2976,2925,2994,4192,3499]
[600,3719,3858,3694,3621,3720,5293,4359]
[700,4451,4633,4418,4319,4454,6429,5233]
[800,5192,5418,5150,5021,5195,7599,6122]
[900,5940,6212,5889,5725,5945,8790,7025]
[1000,6695,7015,6635,6433,6702,10015,7944]
[1100,7459,7826,7399,7145,7467,11263,8880]
[1200,8230,8645,8151,7861,8239,12533,9831]
[1300,9010,9471,8922,8581,9021,13820,10799]
[1400,9797,10304,9699,9306,9809,15122,11783]
[1500,10590,11142,10485,10035,10606,16436,12783]
[1600,11392,11988,11278,10769,11409,17773,13798]
[1700,12200,12836,12080,11509,12220,19119,14831]
[1800,13016,13691,12888,12254,13036,20469,15877]
[1900,13837,14551,13702,13003,13858,21840,16941]
[2000,14663,15415,14524,13759,14688,23211,18019]

{"sheet":"B11","index":2,"n_rows":28,"n_cols":4,"rows_kept":28,"cut":false,"hidden":true,"merged":[[2,1,2,3]]}
["Integral Heats of Solution and Mixing at 25°C"]
[]
[null,"ΔĤs (kJ/mol)"]
["r (moleH2O/mol solute)","HCl (g)","NaOH (s)","H2SO4"]
[0.5,null,null,-15.73]
[1,-26.22,null,-28.07]
[1.5,null,null,-36.9]
[2,-48.82,null,-41.92]
[3,-56.85,-28.87,-48.99]
[4,-61.2,-34.43,-54.06]
[5,-64.05,-37.74,-58.03]
[10,-69.489999999999995,-42.51,-67.03]
[20,-71.78,-42.84]
[25,null,null,-72.3]
[30,-72.59,-42.72]
[40,-73,-42.59]
[50,-73.260000000000005,-42.51,-73.34]
[100,-73.849999999999994,-42.34,-73.97]
[200,-74.2,-42.26]
[500,-74.52,-42.38,-76.73]
[1000,-74.680000000000007,-42.47,-78.569999999999993]
[2000,-74.819999999999993,-42.55]
[5000,-74.930000000000007,-42.68,-84.43]
[10000,-74.989999999999995,-42.72,-87.07]
[50000,-75.08,-42.8]
[100000,-75.099999999999994,null,-93.64]
[500000,null,null,-95.31]
["infinity",-75.14,-42.89,-96.19]

{"sheet":"Atomic","index":3,"n_rows":119,"n_cols":6,"rows_kept":119,"cut":false,"hidden":true,"merged":[]}
[]
[null,"Atomic Number","Symbol","Element","Atomic Weight","Unstable"]
[null,89,"Ac","Actinium",227,1]
[null,13,"Al","Aluminium",26.9815]
[null,95,"Am","Americium",243,1]
[null,51,"Sb","Antimony",121.75]
[null,18,"Ar","Argon",39.948]
[null,33,"As","Arsenic",74.921599999999998]
[null,85,"At","Astatine",210,1]
[null,56,"Ba","Barium",137.34]
[null,97,"Bk","Berkelium",247,1]
[null,4,"Be","Beryllium",9.0122]
[null,83,"Bi","Bismuth",208.98]
[null,107,"Bh","Bohrium",272,1]
[null,5,"B","Boron",10.811]
[null,35,"Br","Bromine",79.903999999999996]
[null,48,"Cd","Cadmium",112.4]
[null,20,"Ca","Calcium",40.08]
[null,98,"Cf","Californium",251,1]
[null,6,"C","Carbon",12.011150000000001]
[null,58,"Ce","Cerium",140.12]
[null,55,"Cs","Cesium",132.905]
[null,17,"Cl","Chlorine",35.453000000000003]
[null,24,"Cr","Chromium",51.996000000000002]
[null,27,"Co","Cobalt",58.933194999999998]
[null,29,"Cu","Copper",63.545999999999999]
[null,96,"Cm","Curium",247,1]
[null,110,"Ds","Darmstadtium",281,1]
[null,105,"Db","Dubnium",268,1]
[null,66,"Dy","Dysprosium",162.5]
[null,99,"Es","Einsteinium",252,1]
[null,68,"Er","Erbium",167.26]
[null,63,"Eu","Europium",151.96]
[null,100,"Fm","Fermium",257,1]
[null,9,"F","Fluorine",18.998403199999998]
[null,87,"Fr","Francium",223,1]
[null,64,"Gd","Gadolinium",157.25]
[null,31,"Ga","Gallium",69.72]
[null,32,"Ge","Germanium",72.59]
[null,79,"Au","Gold",196.96700000000001]
[null,72,"Hf","Hafnium",178.49]
[null,108,"Hs","Hassium",270,1]
[null,2,"He","Helium",4.0026000000000002]
[null,67,"Ho","Holmium",164.93]
[null,1,"H","Hydrogen",1.00797]
[null,49,"In","Indium",114.82]
[null,53,"I","Iodine",126.9044]
[null,77,"Ir","Iridium",192.22]
[null,26,"Fe","Iron",55.847000000000001]
[null,36,"Kr","Krypton",83.8]
[null,57,"La","Lanthanum",138.91]
[null,103,"Lr","Lawrencium",262,1]
[null,82,"Pb","Lead",207.19]
[null,3,"Li","Lithium",6.9390000000000001]
[null,71,"Lu","Lutetium",174.97]
[null,12,"Mg","Magnesium",24.312000000000001]
[null,25,"Mn","Manganese",54.938000000000002]
[null,109,"Mt","Meitnerium",276,1]
[null,101,"Md","Mendelevium",258,1]
[null,80,"Hg","Mercury",200.59]
[null,42,"Mo","Molybdenum",95.94]
[null,60,"Nd","Neodymium",144.24]
[null,10,"Ne","Neon",20.183]
[null,93,"Np","Neptunium",237,1]
[null,28,"Ni","Nickel",58.71]
[null,41,"Nb","Niobium",92.906000000000006]
[null,7,"N","Nitrogen",14.0067]
[null,102,"No","Nobelium",259,1]
[null,76,"Os","Osmium",190.2]
[null,8,"O","Oxygen",15.9994]
[null,46,"Pd","Palladium",106.4]
[null,15,"P","Phosphorus",30.973800000000001]
[null,78,"Pt","Platinum",195.09]
[null,94,"Pu","Plutonium",244,1]
[null,84,"Po","Polonium",209,1]
[null,19,"K","Potassium",39.101999999999997]
[null,59,"Pr","Praseodymium",140.90700000000001]
[null,61,"Pm","Promethium",145,1]
[null,91,"Pa","Protactinium",231.03587999999999]
[null,88,"Ra","Radium",226,1]
[null,86,"Rn","Radon",222,1]
[null,75,"Re","Rhenium",186.2]
[null,45,"Rh","Rhodium",102.905]
[null,111,"Rg","Roentgenium",280,1]
[null,37,"Rb","Rubidium",85.47]
[null,44,"Ru","Ruthenium",101.07]
[null,104,"Rf","Rutherfordium",267,1]
[null,62,"Sm","Samarium",150.35]
[null,21,"Sc","Scandium",44.956000000000003]
[null,106,"Sg","Seaborgium",271,1]
[null,34,"Se","Selenium",78.959999999999994]
[null,14,"Si","Silicon",28.085999999999999]
[null,47,"Ag","Silver",107.86799999999999]
[null,11,"Na","Sodium",22.989799999999999]
[null,38,"Sr","Strontium",87.62]
[null,16,"S","Sulfur",32.064]
[null,73,"Ta","Tantalum",180.94800000000001]
[null,43,"Tc","Technetium",98,1]
[null,52,"Te","Tellurium",127.6]
[null,65,"Tb","Terbium",158.92400000000001]
[null,81,"Tl","Thallium",204.37]
[null,90,"Th","Thorium",232.03800000000001]
[null,69,"Tm","Thulium",168.934]
[null,50,"Sn","Tin",118.69]
[null,22,"Ti","Titanium",47.9]
[null,74,"W","Tungsten",183.85]
[null,112,"Uub","Ununbium",285,1]
[null,116,"Uuh","Ununhexium",293,1]
[null,118,"Uuo","Ununoctium",294,1]
[null,115,"Uup","Ununpentium",288,1]
[null,114,"Uuq","Ununquadium",289,1]
[null,113,"Uut","Ununtrium",284,1]
[null,92,"U","Uranium",238.03]
[null,23,"V","Vanadium",50.942]
[null,54,"Xe","Xenon",131.30000000000001]
[null,70,"Yb","Ytterbium",173.04]
[null,39,"Y","Yttrium",88.905000000000001]
[null,30,"Zn","Zinc",65.37]
[null,40,"Zr","Zirconium",91.22]

{"sheet":"ANTOINE","index":4,"n_rows":99,"n_cols":7,"rows_kept":99,"cut":false,"hidden":true,"merged":[]}
["Antione Equation Constants"]
[]
[]
["Compound","Formula","Lower Temp °C","Upper Temp °C","A","B","C"]
["1,1,1-Trichloroethane","C2H3Cl3",-5.4,16.899999999999999,8.64344,2136.6210000000001,302.76900000000001]
["1,1,2-Trichloroethane","C2H3Cl3",50,113.7,6.9518500000000003,1314.41,209.197]
["1,1-Dichloroethane","C2H4Cl2",-38.799999999999997,17.600000000000001,6.9770200000000004,1174.0219999999999,229.06]
["1,2-Dichloroethane","C2H4Cl",-30.8,99.4,7.0252999999999997,1271.2539999999999,222.92699999999999]
["1,2-Ethylenediamine","C2H8N2",26.5,117.4,7.1687099999999999,1336.2349999999999,194.36600000000001]
["1,4-Dioxane","C4H8O2",20,105,7.4315499999999997,1554.6790000000001,240.33699999999999]
["1-Butanol","C4H10O",89.2,125.7,7.3636600000000003,1305.1980000000001,173.42699999999999]
["1-Butene","C4H8",-77.5,-3.7,6.5310100000000002,810.26099999999997,228.066]
["1-Decene","C10H20",86.8,171.6,6.9543299999999997,1497.527,197.05600000000001]
["1-Heptene","C7H14",21.6,94.5,6.9138099999999998,1265.1199999999999,220.05099999999999]
["1-Hexene","C6H12",15.9,64.3,6.8688000000000002,1154.646,226.04599999999999]
["1-Nonene","C9H18",66.599999999999994,147.9,6.95777,1437.8620000000001,205.81399999999999]
["1-Octene","C8H16",44.9,122.2,6.9363700000000001,1355.779,213.02199999999999]
["1-Pentanol","C5H12O",74.7,156,7.1824599999999998,1287.625,161.33000000000001]
["1-Pentene","C5H10",12.8,30.7,6.8426799999999997,1043.2059999999999,233.34399999999999]
["1-Propanol","C3H8O",60.2,104.6,7.7441599999999999,1437.6859999999999,198.46299999999999]
["2-Butanol","C4H10O",72.400000000000006,107.1,7.2013100000000003,1157,168.279]
["2-Propanol","C3H8O",52.3,89.3,7.7402100000000003,1359.5170000000001,197.52699999999999]
["Acetaldehyde","C2H4O",-0.2,34.4,8.0055200000000006,1600.0017,291.80900000000003]
["Acetic acid","C2H4O2",29.8,126.5,7.3878199999999996,1533.3130000000001,222.309]
["Acetic acid","C2H4O2",0,36,7.1880699999999997,1416.7,225]
["Acetic anhydride","C4H6O3",62.8,139.4,7.1494799999999996,1444.7180000000001,199.81700000000001]
["Acetone","C3H6O",-12.9,55.3,7.11714,1210.595,229.66399999999999]
["Acrylic acid","C3H4O2",20,70,5.6520400000000004,648.62900000000002,154.68299999999999]
["Ammonia","NH3",-83,60,7.5546600000000002,1002.711,247.88499999999999]
["Aniline","C6H7N",102.6,185.2,7.3201000000000001,1731.5150000000001,206.04900000000001]
["Benzene","C6H6",14.5,80.900000000000006,6.8927199999999997,1203.5309999999999,219.88800000000001]
["Butyric acid","C4H8O2",20,150,8.7101900000000008,2433.0140000000001,255.18899999999999]
["Carbon disulfide","CS2",3.6,79.900000000000006,6.9427899999999996,1169.1099999999999,241.59299999999999]
["Carbon tetrachloride","CCl4",14.1,76,6.8792600000000004,1212.021,226.40899999999999]
["Chlorobenzene","C6H5Cl",62,131.69999999999999,6.9780800000000003,1431.0530000000001,217.55]
["Chlorobenzene","C6H5Cl",0,42,7.1069000000000004,1500,224]
["Chlorobenzene","C6H5Cl",42,230,6.9450399999999997,1413.12,216]
["Chloroform","CHCl3",-10.4,60.3,6.95465,1170.9659999999999,226.232]
["Chloroform","CHCl3",-30,150,6.9032799999999996,1163.03,227.4]
["Cyclohexane","C6H12",19.899999999999999,81.599999999999994,6.8494099999999998,1206.001,223.148]
["Cyclohexanol","C6H12O",93.7,160.69999999999999,6.2553000000000001,912.86599999999999,109.126]
["Dichloromethane","CH2Cl2",-40,40,7.40916,1325.9380000000001,252.61600000000001]
["Diethyl ether","C4H10O",-60.8,19.899999999999999,6.9203200000000002,1064.066,228.79900000000001]
["Diethyl ketone","C5H10O",56.5,111.3,7.02529,1310.2809999999999,214.19200000000001]
["Diethylene glycol","C4H10O2",130,243,7.63666,1939.3589999999999,162.714]
["Dimethyl ether","C2H6O",-78.2,-24.9,6.9760299999999997,889.26400000000001,241.95699999999999]
["Dimethylamine","C2H7N",-71.8,6.9,7.0821199999999997,960.24199999999996,221.667]
["Ethanol","C2H6O",19.600000000000001,93.4,8.1121999999999996,1592.864,226.184]
["Ethanolamine","C2H7NO",65.400000000000006,170.9,7.4568000000000003,1577.67,173.36799999999999]
["Ethyl acetate","C4H8O2",15.6,75.8,7.1017900000000003,1244.951,217.881]
["Ethyl acetate","C4H8O2",-20,150,7.0980800000000004,1238.71,217]
["Ethyl chloride","C2H5Cl",-55.9,12.5,6.9864699999999997,1030.0070000000001,238.61199999999999]
["Ethylbenzene","C8H10",56.5,137.1,6.9565000000000001,1423.5429999999999,213.09100000000001]
["Ethylene glycol","C2H6O2",50,200,8.0908300000000004,2088.9360000000001,203.45400000000001]
["Ethylene oxide","C2H4O",0.3,31.8,8.6901600000000006,2005.779,334.76499999999999]
["Formaldehyde","HCHO",-109.4,-22.3,7.1957800000000001,970.59500000000003,244.124]
["Formic acid","CH2O2",37.4,100.7,7.5817800000000002,1699.173,260.714]
["Glycerol","C3H8O3",183.3,260.39999999999998,6.1650099999999997,1036.056,28.097000000000001]
["Hydrogen Cyanide","HCN",-16.399999999999999,46.2,7.5282299999999998,1329.49,260.41800000000001]
["i-Butane","C4H10",-85.1,-11.6,6.7886600000000001,899.61699999999996,241.94200000000001]
["i-Heptane","C7H16",18.5,90.9,6.8768900000000004,1238.1220000000001,219.78299999999999]
["i-Hexane","C6H14",12.8,61.1,6.8683899999999998,1151.4010000000001,228.477]
["i-Octane","C8H18",41.7,118.5,6.8881399999999999,1319.529,211.625]
["i-Pentane","C5H12",16.3,28.6,6.7345699999999997,992.01900000000001,229.56399999999999]
["Methanol","CH3OH",14.9,83.7,8.0809700000000007,1582.271,239.726]
["Methanol","CH3OH",-20,140,7.8786300000000002,1473.11,230]
["Methyl acetate","C3H6O2",1.8,55.8,7.0652400000000002,1157.6300000000001,219.726]
["Methyl bromide","CH3Br",-70,3.6,7.09084,1046.066,244.91399999999999]
["Methyl chloride","CH3Cl",-75,5,7.0934900000000001,948.58199999999999,249.33600000000001]
["Methyl ethyl ketone","C4H8O",42.8,88.4,7.0635599999999998,1261.3389999999999,221.96899999999999]
["Methyl isobutyl ketone","C6H12O",21.7,116.2,6.67272,1168.4079999999999,191.94399999999999]
["Methyl methacrylate","C5H8O2",39.200000000000003,89.2,8.4091900000000006,2050.4670000000001,274.36900000000003]
["Methylamine","CH5N",-83.1,-6.2,7.3369,1011.532,233.286]
["Methylcyclohexane","C7H14",25.6,101.8,6.8282699999999998,1273.673,221.72300000000001]
["m-Xylene","C8H10",59.2,140,7.0064599999999997,1460.183,214.827]
["N,N-Dimethylformamide","C3H7NO",30,90,6.9279599999999997,1400.8689999999999,196.434]
["Naphthalene","C10H8",80.3,179.5,7.0335799999999997,1756.328,204.84200000000001]
["n-Butane","C4H10",-78,-0.3,6.8248499999999996,943.45299999999997,239.71100000000001]
["n-Decane","C10H22",94.5,175.1,6.9570699999999999,1503.568,194.738]
["n-Heptane","C7H16",25.9,99.3,6.9025299999999996,1267.828,216.82300000000001]
["n-Hexane","C6H14",13,69.5,6.8855500000000003,1175.817,224.86699999999999]
["Nitrobenzene","C6H5NO2",134.1,210.6,7.1156199999999998,1746.586,201.78299999999999]
["Nitromethane","CH3NO2",55.7,136.4,7.2816599999999996,1446.9369999999999,227.6]
["n-Nonane","C9H20",70.3,151.80000000000001,6.93764,1430.4590000000001,201.80799999999999]
["n-Octane","C8H18",52.9,126.6,6.9187399999999997,1351.7560000000001,209.1]
["n-Pentane","C5H12",13.3,36.799999999999997,6.8447100000000001,1060.7929999999999,231.541]
["o-Xylene","C8H10",63.5,145.4,7.0015400000000003,1476.393,213.87200000000001]
["Phenol","C6H6O",107.2,181.8,7.1330099999999996,1516.79,174.95400000000001]
["Propionic acid","C3H6O2",72.400000000000006,128.30000000000001,7.7142299999999997,1733.4179999999999,217.72399999999999]
["Propylene oxide","C3H6O",-24.2,34.799999999999997,7.0144299999999999,1086.3689999999999,228.59399999999999]
["p-Xylene","C8H10",58.3,139.30000000000001,6.9882,1451.7919999999999,215.11099999999999]
["Pyridine","C5H5N",67.3,152.9,7.04115,1373.799,214.97900000000001]
["Styrene","C8H8",29.9,144.80000000000001,7.06623,1507.434,214.98500000000001]
["Toluene","C7H8",35.299999999999997,111.5,6.9580500000000001,1346.7729999999999,219.69300000000001]
["Trichoroethylene","C2HCl3",17.8,86.5,6.5182700000000002,1018.603,192.73099999999999]
["Vinyl acetate","C4H6O2",21.8,72,7.2100999999999997,1296.1300000000001,226.655]
["Water","H2O",0,60,8.1076499999999996,1750.2860000000001,235]
["Water","H2O",60,150,7.9668099999999997,1668.21,228]
["ZZZ"]

{"sheet":"KOPPS","index":5,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":true,"merged":[[3,1,3,2]]}
["Atomic Heat Capacities for Kopp's Rule"]
[]
[]
[null,"Cpa (J/(g-atom°C))"]
["Element","Solids","Liquids"]
["B",11,20]
["C",7.5,12]
["F",21,29]
["H",9.6,18]
["O",17,25,null,"C",1]
["P",23,31,null,"H",4]
["S",26,31,null,"N",2]
["Si",16,24]
["ZZ",26,33,null,null,{"$f":"[0]!Kopps(E10:E12,F10:F12,\"L\")","v":{"$error":"#VALUE!"}}]

{"sheet":"B3","index":6,"n_rows":88,"n_cols":12,"rows_kept":88,"cut":false,"hidden":true,"merged":[]}
["Vapor Pressure of Water"]
[]
["Pv (mmHg) versus T (°C)"]
[]
[null,"T (°C)",0,0.1,0.2,0.3,0.4,0.5,0.6,0.7,0.8,0.9]
[null,-14,1.361,1.3480000000000001,1.3360000000000001,1.3240000000000001,1.3120000000000001,1.3,1.288,1.276,1.264,1.2529999999999999]
[null,-13,1.49,1.4770000000000001,1.464,1.45,1.4370000000000001,1.4239999999999999,1.411,1.399,1.3859999999999999,1.373]
[null,-12,1.6319999999999999,1.617,1.6020000000000001,1.5880000000000001,1.5740000000000001,1.5589999999999999,1.546,1.532,1.518,1.504]
[null,-11,1.7849999999999999,1.7689999999999999,1.7529999999999999,1.7370000000000001,1.722,1.7070000000000001,1.6910000000000001,1.6759999999999999,1.661,1.6459999999999999]
[null,-10,1.95,1.9339999999999999,1.9159999999999999,1.899,1.883,1.8660000000000001,1.849,1.833,1.8169999999999999,1.8]
[null,-9,2.1309999999999998,2.1219999999999999,2.093,2.0750000000000002,2.0569999999999999,2.0390000000000001,2.0209999999999999,2.0030000000000001,1.9850000000000001,1.968]
[null,-8,2.3260000000000001,2.306,2.2850000000000001,2.266,2.246,2.226,2.2069999999999999,2.1869999999999998,2.1680000000000001,2.149]
[null,-7,2.5369999999999999,2.5150000000000001,2.4929999999999999,2.472,2.4500000000000002,2.4289999999999998,2.4079999999999999,2.387,2.367,2.3460000000000001]
[null,-6,2.7650000000000001,2.742,2.718,2.6949999999999998,2.6720000000000002,2.649,2.6259999999999999,2.6030000000000002,2.581,2.5590000000000002]
[null,-5,3.0129999999999999,2.9870000000000001,2.9620000000000002,2.9369999999999998,2.9119999999999999,2.887,2.8620000000000001,2.8380000000000001,2.8130000000000002,2.79]
[null,-4,3.28,3.2519999999999998,3.2250000000000001,3.198,3.1709999999999998,3.1440000000000001,3.117,3.0910000000000002,3.0649999999999999,3.0390000000000001]
[null,-3,3.5680000000000001,3.5390000000000001,3.5089999999999999,3.48,3.4510000000000001,3.4220000000000002,3.3929999999999998,3.3639999999999999,3.3359999999999999,3.3079999999999998]
[null,-2,3.88,3.8479999999999999,3.8159999999999998,3.7850000000000001,3.7530000000000001,3.722,3.6909999999999998,3.66,3.63,3.5990000000000002]
[null,-1,4.2169999999999996,4.1820000000000004,4.1470000000000002,4.1130000000000004,4.0789999999999997,4.0449999999999999,4.0119999999999996,3.9790000000000001,3.9460000000000002,3.9129999999999998]
["Ice",0,4.5789999999999997,4.5419999999999998,4.5039999999999996,4.4669999999999996,4.431,4.3949999999999996,4.359,4.3230000000000004,4.2869999999999999,4.2519999999999998]
["Liquid Water",0,4.5789999999999997,4.6130000000000004,4.6470000000000002,4.681,4.7149999999999999,4.75,4.7850000000000001,4.82,4.8550000000000004,4.8899999999999997]
[null,1,4.9260000000000002,4.9619999999999997,4.9980000000000002,5.0339999999999998,5.07,5.1070000000000002,5.1440000000000001,5.181,5.2190000000000003,5.2560000000000002]
[null,2,5.2939999999999996,5.3319999999999999,5.37,5.4080000000000004,5.4470000000000001,5.4859999999999998,5.5250000000000004,5.5650000000000004,5.6050000000000004,5.6449999999999996]
[null,3,5.6849999999999996,5.7249999999999996,5.766,5.8070000000000004,5.8479999999999999,5.8890000000000002,5.931,5.9729999999999999,6.0149999999999997,6.0579999999999998]
[null,4,6.101,6.1440000000000001,6.1870000000000003,6.23,6.274,6.3179999999999996,6.3630000000000004,6.4080000000000004,6.4530000000000003,6.4980000000000002]
[null,5,6.5430000000000001,6.5890000000000004,6.6349999999999998,6.681,6.7279999999999998,6.7750000000000004,6.8220000000000001,6.8689999999999998,6.9169999999999998,6.9649999999999999]
[null,6,7.0129999999999999,7.0620000000000003,7.1109999999999998,7.16,7.2089999999999996,7.2590000000000003,7.3090000000000002,7.36,7.4109999999999996,7.4619999999999997]
[null,7,7.5129999999999999,7.5650000000000004,7.617,7.6689999999999996,7.7220000000000004,7.7750000000000004,7.8280000000000003,7.8819999999999997,7.9359999999999999,7.99]
[null,8,8.0449999999999999,8.1,8.1549999999999994,8.2110000000000003,8.2669999999999995,8.3230000000000004,8.3800000000000008,8.4369999999999994,8.4939999999999998,8.5510000000000002]
[null,9,8.609,8.6679999999999993,8.7270000000000003,8.7859999999999996,8.8450000000000006,8.9049999999999994,8.9649999999999999,9.0250000000000004,9.0860000000000003,9.1470000000000002]
[null,10,9.2089999999999996,9.2710000000000008,9.3330000000000002,9.3949999999999996,9.4580000000000002,9.5210000000000008,9.5850000000000009,9.6489999999999991,9.7140000000000004,9.7789999999999999]
[null,11,9.8439999999999994,9.91,9.9760000000000009,10.042,10.109,10.176,10.244,10.311999999999999,10.38,10.449]
[null,12,10.518000000000001,10.587999999999999,10.657999999999999,10.728,10.798999999999999,10.87,10.941000000000001,11.013,11.085000000000001,11.157999999999999]
[null,13,11.231,11.305,11.379,11.452999999999999,11.528,11.603999999999999,11.68,11.756,11.833,11.91]
[null,14,11.987,12.065,12.144,12.223000000000001,12.302,12.382,12.462,12.542999999999999,12.624000000000001,12.706]
[null,15,12.788,12.87,12.952999999999999,13.037000000000001,13.121,13.205,13.29,13.375,13.461,13.547000000000001]
[null,16,13.634,13.721,13.808999999999999,13.898,13.987,14.076000000000001,14.166,14.256,14.347,14.438000000000001]
[null,17,14.53,14.622,14.715,14.808999999999999,14.903,14.997,15.092000000000001,15.188000000000001,15.284000000000001,15.38]
[null,18,15.477,15.574999999999999,15.673,15.772,15.871,15.971,16.071000000000002,16.170999999999999,16.271999999999998,16.373999999999999]
[null,19,16.477,16.581,16.684999999999999,16.789000000000001,16.893999999999998,16.998999999999999,17.105,17.212,17.318999999999999,17.427]
[null,20,17.535,17.643999999999998,17.753,17.863,17.974,18.085000000000001,18.196999999999999,18.309000000000001,18.422000000000001,18.536000000000001]
[null,21,18.649999999999999,18.765000000000001,18.88,18.995999999999999,19.113,19.231000000000002,19.349,19.468,19.587,19.707000000000001]
[null,22,19.827000000000002,19.948,20.07,20.193000000000001,20.315999999999999,20.440000000000001,20.565000000000001,20.69,20.815000000000001,20.940999999999999]
[null,23,21.068000000000001,21.196000000000002,21.324000000000002,21.452999999999999,21.582999999999998,21.713999999999999,21.844999999999999,21.977,22.11,22.242999999999999]
[null,24,22.376999999999999,22.512,22.648,22.785,22.922000000000001,23.06,23.198,23.337,23.475999999999999,23.616]
[null,25,23.756,23.896999999999998,24.039000000000001,24.181999999999999,24.326000000000001,24.471,24.617000000000001,24.763999999999999,24.911999999999999,25.06]
[null,26,25.209,25.359000000000002,25.509,25.66,25.812000000000001,25.963999999999999,26.117000000000001,26.271000000000001,26.425999999999998,26.582000000000001]
[null,27,26.739000000000001,26.896999999999998,27.055,27.213999999999999,27.373999999999999,27.535,27.696000000000002,27.858000000000001,28.021000000000001,28.184999999999999]
[null,28,28.349,28.513999999999999,28.68,28.847000000000001,29.015000000000001,29.184000000000001,29.353999999999999,29.524999999999999,29.696999999999999,29.87]
[null,29,30.042999999999999,30.216999999999999,30.391999999999999,30.568000000000001,30.745000000000001,30.922999999999998,31.102,31.280999999999999,31.460999999999999,31.641999999999999]
[null,30,31.824000000000002,32.006999999999998,32.191000000000003,32.375999999999998,32.561,32.747,32.933999999999997,33.122,33.311999999999998,33.503]
[null,31,33.695,33.887999999999998,34.082000000000001,34.276000000000003,34.470999999999997,34.667000000000002,34.863999999999997,35.061999999999998,35.261000000000003,35.462000000000003]
[null,32,35.662999999999997,35.865000000000002,36.067999999999998,36.271999999999998,36.476999999999997,36.683,36.890999999999998,37.098999999999997,37.308,37.518000000000001]
[null,33,37.728999999999999,37.942,38.155000000000001,38.369,38.584000000000003,38.801000000000002,38.018000000000001,39.237000000000002,39.457000000000001,39.677]
[null,34,39.898000000000003,40.121000000000002,40.344000000000001,40.569000000000003,40.795999999999999,41.023000000000003,41.250999999999998,41.48,41.71,41.942]
[null,35,42.174999999999997,42.408999999999999,42.643999999999998,42.88,43.116999999999997,43.354999999999997,43.594999999999999,43.835999999999999,44.078000000000003,44.32]
[null,36,44.563000000000002,44.808,45.054000000000002,45.301000000000002,45.548999999999999,45.798999999999999,46.05,46.302,46.555999999999997,46.811]
[null,37,47.067,47.323999999999998,47.582000000000001,47.841000000000001,48.101999999999997,48.363999999999997,48.627000000000002,48.890999999999998,49.156999999999996,49.423999999999999]
[null,38,49.692,49.960999999999999,50.231000000000002,50.502000000000002,50.774000000000001,51.048000000000002,51.323,51.6,51.878999999999998,52.16]
[null,39,52.442,52.725000000000001,53.009,53.293999999999997,53.58,53.866999999999997,54.155999999999999,54.445999999999998,54.737000000000002,55.03]
[null,40,55.323999999999998,55.61,55.91,56.21,56.51,56.81,57.11,57.41,57.72,58.03]
[null,41,58.34,58.65,58.96,59.27,59.58,59.9,60.22,60.54,60.86,61.18]
[null,42,61.5,61.82,62.14,62.47,62.8,63.13,63.46,63.79,64.12,64.459999999999994]
[null,43,64.8,65.14,65.48,65.819999999999993,66.16,66.510000000000005,66.86,67.209999999999994,67.56,67.91]
[null,44,68.260000000000005,68.61,68.97,69.33,69.69,70.05,70.41,70.77,71.14,71.510000000000005]
[null,45,71.88,72.25,72.62,72.989999999999995,73.36,73.739999999999995,74.12,74.5,74.88,75.260000000000005]
[null,46,75.650000000000006,76.040000000000006,76.430000000000007,76.819999999999993,77.209999999999994,77.599999999999994,78,78.400000000000006,78.8,79.2]
[null,47,79.599999999999994,80,80.41,80.819999999999993,81.23,81.64,82.05,82.46,82.87,83.29]
[null,48,83.71,84.13,84.56,84.99,85.42,85.85,86.28,86.71,87.14,87.58]
[null,49,88.02,88.46,88.9,89.34,89.79,90.24,90.69,91.14,91.59,92.05]
[null,"T (°C)",0,1,2,3,4,5,6,7,8,9]
[null,50,92.51,97.2,102.09,107.2,112.51,118.04,123.8,129.82,136.08000000000001,142.6]
[null,60,149.38,156.43,163.77000000000001,171.38,179.31,187.54,196.09,204.96,214.17,223.73]
[null,70,233.7,243.9,254.6,265.7,277.2,289.10000000000002,301.39999999999998,314.10000000000002,327.3,341]
[null,80,355.1,369.7,384.9,400.6,416.8,433.6,450.9,468.7,487.1,506.1]
[null,"T (°C)",0,0.1,0.2,0.3,0.4,0.5,0.6,0.7,0.8,0.9]
[null,90,525.76,527.76,529.77,531.78,533.79999999999995,535.82000000000005,537.86,539.9,541.95000000000005,544]
[null,91,546.04999999999995,548.11,550.17999999999995,552.26,554.35,556.44000000000005,558.53,560.64,562.75,564.87]
[null,92,566.99,569.12,571.26,573.4,575.54999999999995,577.71,579.87,582.04,584.22,586.41]
[null,93,588.6,590.79999999999995,593,595.21,597.42999999999995,599.66,601.89,604.13,606.38,608.64]
[null,94,610.9,613.16999999999996,615.44000000000005,617.72,620.01,622.30999999999995,624.61,626.91999999999996,629.24,631.57000000000005]
[null,95,633.9,636.24,638.59,640.94000000000005,643.29999999999995,645.66999999999996,648.04999999999995,650.42999999999995,652.82000000000005,655.22]
[null,96,657.62,660.03,662.45,664.88,667.31,669.75,672.2,674.66,677.12,679.69]
[null,97,682.07,684.55,687.04,689.54,692.05,694.57,697.1,699.63,702.17,704.71]
[null,98,707.27,709.83,712.4,714.98,717.56,720.15,722.75,725.36,727.98,730.61]
[null,99,733.24,735.88,738.53,741.18,743.85,746.52,749.2,751.89,754.58,757.29]
[null,100,760,762.72,765.45,768.19,770.93,773.68,776.44,779.22,782,784.78]
[null,101,787.57,790.37,793.18,796,798.82,801.66,804.5,807.35,810.21,813.08]

{"sheet":"Sheet1","index":7,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Introduction","index":8,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"Chapter2","index":9,"n_rows":60,"n_cols":18,"rows_kept":60,"cut":false,"hidden":false,"merged":[[36,1,36,2],[36,3,36,4],[36,5,36,6]]}
["Slope examples"]
[]
["Example 1:"]
["A series of meaurement of temperature versus time yields the following points:"]
[]
[null,"x","y"]
[null,0,{"$f":"3.6*B7","v":0}]
[null,2,{"$f":"3.6*B8","v":7.2}]
[null,4,14.4]
[null,6,21.6]
[null,7,25.2]
[null,8,28.8]
[null,10,36]
[null,12,43.2]
[null,14,50.4]
[null,16,57.6]
[null,18,64.8]
[null,20,72]
[]
["If the value of x is 7.89, what is the value of y?"]
[]
["Solution:"]
[null,"using vba function",null,null,"using microsoft excel:"]
[null,"slope =",{"$f":"[0]!Slope1(C7:C18,B7:B18)","v":3.5999999999999996},null,"slope=",{"$f":"SLOPE(C7:C18,B7:B18)","v":3.5999999999999996}]
[null,null,null,null,"intercept=",{"$f":"INTERCEPT(C7:C18,B7:B18)","v":7.1054273576010019E-15}]
[null,"using slope intercept form to find y : y=slope *x"]
[]
[null,"y=",{"$f":"C24*7.89","v":28.403999999999996}]
[]
[]
[]
[]
[]
["Example 2:"]
["(Problem 2.42 from Elementary Priciples of Chemical Processes)",null,null,null,null,null,null,null,null,"Test Yourself, Problem 1, P. 23"]
[null,null,null,null,null,null,null,null,null,null,"f","t"]
[null,"Lab 1",null,"Lab 2",null,"Lab3",null,null,null,null,1,1]
[null,"T= 275°C",null,"T=275°C",null,"T=275°C",null,null,null,null,4,2]
[null,"CA0 (g/L) ",null,"CA0 (g/L) ",null,"CA0 (g/L) ",null,null,null,null,8,3]
[null,4.83,"Linearized",5.14,"Linearized",3.69,"Linearized"]
["t(s)","Cp(g/L)","data","Cp(g/L)","data","Cp(g/L)","data"]
[0,0,{"$f":"LN(1-B42/$B$40)","v":0},0,{"$f":"LN(1-D42/$D$40)","v":0},0,{"$f":"LN(1-F42/$F$40)","v":0},null,null,null,null,"f(t=1.3)=",{"$f":"[0]!linterp(L37:L39,K37:K39,1.3)","v":1.9000000000000001}]
[10,0.28699999999999998,{"$f":"LN(1-B43/$B$40)","v":-6.1258880887215018E-2},0.31,-6.2206611802592432E-2,0.245,-6.8702553586813903E-2,null,null,null,null,"f(f=5)=",{"$f":"[0]!linterp(K37:K39,L37:L39,5)","v":2.25}]
[20,0.59399999999999997,{"$f":"LN(1-B44/$B$40)","v":-0.13122703992532128},0.61399999999999999,-0.12721453225572812,0.46500000000000002,-0.13469350780469996,null,null,null,null,"f(t=5)=",{"$f":"[0]!linterp(L37:L39,K37:K39,5)","v":16}]
[30,0.871,-0.19885499954048777,0.88500000000000001,-0.18895831744173636,0.67,-0.20036962666565752,null,null,null,null,"f(t=0)=",{"$f":"[0]!linterp(L37:L39,K37:K39,0)","v":-2}]
[60,1.51,-0.37488168473608408,1.64,-0.38429011097170573,1.2,-0.39334374757581958]
[120,2.62,-0.78185395213482001,2.66,-0.72879451929018302,2.06,-0.81704644323376496,null,null,"Problem 2.29"]
[240,3.91,-1.6582280766035324,3.87,-1.3980361789965743,3.03,-1.7211419020141012,null,null,null,"The vapor pressure of 1-chlorotetradecane at several temperatures are tabulated here. "]
[360,4.3,-2.2097247401004503,4.6100000000000003,-2.2719313519030448,3.32,-2.2998787313963027]
[480,4.62,-3.1354942159291506,4.8899999999999997,-3.0233474405869631,3.54,-3.202746442938317,null,null,null,null,"T (°C)",98.5,131.80000000000001,148.19999999999999,166.2,199.8,215.5]
[600,4.68,-3.4719664525503608,5.03,-3.8443279926567979,3.59,-3.6082115510464803,null,null,null,null,"p* (mmHg)",1,5,10,20,60,100]
[]
["Solution:",null,null,null,null,null,null,null,null,null,"Use two-point linear interpolation to estimate the value of p* at T=185°C"]
["Single Parameter Slope",null,null,null,null,"Two parameter slope"]
[null,"Lab 1","Lab 2","Lab 3",null,"Lab 1","Lab 2","Lab 3",null,"Solution:"]
[null,{"$f":"[0]!Slope1(C42:C51,A42:A51)","v":-6.1571027539914112E-3},{"$f":"[0]!Slope1(E42:E51,A42:A51)","v":-6.3118888230609934E-3},{"$f":"[0]!Slope1(G42:G51,A42:A51)","v":-6.3667676355820156E-3},null,{"$f":"SLOPE(C42:C51,A42:A51)","v":-6.0666280856964475E-3},{"$f":"SLOPE(E42:E51,A42:A51)","v":-6.3521029910490927E-3},{"$f":"SLOPE(G42:G51,A42:A51)","v":-6.2672891501460697E-3},null,null,"T=",185,"°C"]
[null,null,null,null,null,null,null,null,null,null,"p*=",{"$f":"[0]!linterp(M50:R50,M51:R51,L56)","v":42.38095238095238},"mmHg"]
["%Error from using 2 parameter slope function:"]
[null,"Lab 1","Lab 2","Lab 3"]
[null,{"$f":"(F56-B56)/B56","v":-1.4694357380394948E-2},{"$f":"(G56-C56)/C56","v":6.3711781236028197E-3},-1.5624645209287909E-2]

{"sheet":"Chapter 3","index":10,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[[30,0,30,1]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Molecular Weights"]
[null,"MW","Acetone",{"$f":"[0]!MW(\"Acetone\")","v":{"$error":"#VALUE!"}},{"$f":"[0]!MW(C16)","v":{"$error":"#VALUE!"}}]
[null,null,"Mercury",{"$f":"[0]!MW(\"Mercury\")","v":{"$error":"#VALUE!"}},{"$f":"[0]!MW(C17)","v":{"$error":"#VALUE!"}}]
[null,null,"Water",{"$f":"[0]!MW(\"water\")","v":{"$error":"#VALUE!"}},{"$f":"[0]!MW(C18)","v":{"$error":"#VALUE!"}}]
[]
[]
[null,null,null,null,null,"H",2]
[null,null,null,null,null,"O",1]
[null,null,null,null,"MW of H2O",{"$f":"[0]!MWCalc(F21:F22,G21:G22)","v":{"$error":"#VALUE!"}},{"$f":"F23","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,"hydrogen",2]
[null,null,null,null,null,"oxygen",1]
[null,null,null,null,"MW of H2O",{"$f":"[0]!MWCalc(F24:F25,G24:G25)","v":{"$error":"#VALUE!"}}]
[]
[]
[]
[null,"Specific Gravity",null,null,"SG","Density"]
["rref",null,null,null,null,"lbm/ft3","g/cm3","kg/m3"]
[62.4,"lbm/ft3","Acetone",null,{"$f":"[0]!SG(C32)","v":{"$error":"#VALUE!"}},{"$f":"E32*$A$32","v":{"$error":"#VALUE!"}},{"$f":"E32*$A$33","v":{"$error":"#VALUE!"}},{"$f":"E32*$A$34","v":{"$error":"#VALUE!"}}]
[1,"g/cm3","Mercury",null,{"$f":"[0]!SG(C33)","v":{"$error":"#VALUE!"}},{"$f":"E33*$A$32","v":{"$error":"#VALUE!"}},{"$f":"E33*$A$33","v":{"$error":"#VALUE!"}}]
[1000,"kg/m3","methyl amine",null,{"$f":"[0]!SG(C34)","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[1,"kg/L"]
[1,"ton/m3"]
[1,"g/mL"]

{"sheet":"Chapter 4","index":11,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Chapter 5","index":12,"n_rows":16,"n_cols":17,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Function","Trial of Function"]
[null,null,null,null,null,null,null,null,null,null,null,null,"MW","Acetone=",{"$f":"[0]!MW(\"Acetone\")","v":{"$error":"#VALUE!"}},"Mercury=",{"$f":"[0]!MW(\"Mercury\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,"SG","Acetone=",{"$f":"[0]!SG(\"Acetone\")","v":{"$error":"#VALUE!"}},"Mercury=",{"$f":"[0]!SG(\"Mercury\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Tm","Acetone=",{"$f":"[0]!Tm(\"Acetone\")","v":{"$error":"#VALUE!"}},"Mercury=",{"$f":"[0]!Tm(\"Mercury\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Hm","Acetone=",{"$f":"[0]!Hm(\"acetone\")","v":{"$error":"#VALUE!"}},"Carbon (Graphite)=",{"$f":"[0]!Hm(\"carbon\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Tb","Acetone=",{"$f":"[0]!tb(\"acetone\")","v":{"$error":"#VALUE!"}},"Mercury=",{"$f":"[0]!tb(\"mercury\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Decomp","Acetone=",{"$f":"[0]!Decomp(\"acetone\")","v":{"$error":"#VALUE!"}},"Ammonium Nitrate=",{"$f":"[0]!Decomp(\"Ammonium nitrate\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Sublim","Acetone=",{"$f":"[0]!Sublim(\"acetone\")","v":{"$error":"#VALUE!"}},"Carbon dioxide=",{"$f":"[0]!Sublim(\"carbon dioxide\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Ignite","Acetone=",{"$f":"[0]!Ignite(\"acetone\")","v":{"$error":"#VALUE!"}},"Phosphorus (red)=",{"$f":"[0]!Ignite(\"Phosphorus (red)\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Hv","Acetone=",{"$f":"[0]!Hv(\"acetone\")","v":{"$error":"#VALUE!"}},"Methane=",{"$f":"[0]!Hv(\"methane\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Tcrit","Acetone=",{"$f":"[0]!Tcrit(\"acetone\")","v":{"$error":"#VALUE!"}},"Methane=",{"$f":"[0]!Tcrit(\"methane\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Pcrit","Acetone=",{"$f":"[0]!Pcrit(\"acetone\")","v":{"$error":"#VALUE!"}},"Methane=",{"$f":"[0]!Pcrit(\"methane\")","v":{"$error":"#VALUE!"}}]

{"sheet":"Chapter 6","index":13,"n_rows":100,"n_cols":24,"rows_kept":100,"cut":false,"hidden":false,"merged":[]}
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Example 6.3-3"]
[null,null,null,null,null,null,null,null,null,null,"Example 6.4-3  part 1",null,null,null,null,"Example 6.4-3  part 2"]
[null,null,null,null,null,null,null,null,null,null,"Xbenzene=",0.4,null,null,null,"Ybenzene=",0.1,null,null,null,null,"T(°C) =",75]
[null,null,null,null,null,null,null,null,null,null,"Xtoluene=",0.6,null,null,null,"Ytoluene=",0.1,null,null,null,null,"hr(air)=",0.3]
[null,null,null,null,null,null,null,null,null,null,"Temperature=",368.29596888849397,"K                               or",{"$f":"L6-273.15","v":95.145968888493996},"°C","Temperature=",325.60751425191307,"K           or",{"$f":"Q6-273.15","v":52.457514251913096},"°C",null,"P(mmHg)=",825]
[null,null,null,null,null,null,null,null,null,null,"P*benzene=",{"$f":"[0]!AntoineP(\"Benzene\",L6,\"K\")","v":{"$error":"#VALUE!"}},"mmHg",null,null,"P*benzene=",{"$f":"[0]!AntoineP(\"Benzene\",Q6,\"K\")","v":{"$error":"#VALUE!"}},null,null,null,"(1) Determine the molar flow rates of water, dry air, and oxygen entering the process unit"]
[null,null,null,null,null,null,null,null,null,null,"P*toluene=",{"$f":"[0]!AntoineP(\"Toluene\",L6,\"K\")","v":{"$error":"#VALUE!"}},"mmHg",null,null,"P*toluene=",{"$f":"[0]!AntoineP(\"Toluene\",Q6,\"K\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"p*H2O(mmHg)=",{"$f":"[0]!VPWater(75)","v":{"$error":"#VALUE!"}},{"$f":"Antoine(\"water\",W4)","v":{"$error":"#NAME?"}}]
[null,null,null,null,null,null,null,null,null,null,"f(Tbp)=",{"$f":"L4*L7+L5*L8-760","v":{"$error":"#VALUE!"}},null,null,null,"f(Tdp)=",{"$f":"(Q4*Q12/Q7)+(Q5*Q12/Q8)-1","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"pH2O(mmHg)=",{"$f":"V9*W5","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,"Pbenzene=",{"$f":"L4*L7","v":{"$error":"#VALUE!"}},"mmHg",null,null,"P=",760]
[null,null,null,null,null,null,null,null,null,null,"Ptoluene=",{"$f":"L5*L8","v":{"$error":"#VALUE!"}},"mmHg",null,null,null,null,null,null,null,"yH20=",{"$f":"V11/W6","v":{"$error":"#VALUE!"}},"mol H20/mol"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Xbenzene=",{"$f":"Q4*Q12/Q7","v":{"$error":"#VALUE!"}},"mol Benzene/mol",null,null,"n=",{"$f":"1000*1.1/(348*0.0831)","v":38.037539593620764},"kmol/h"]
[null,null,null,null,null,null,null,null,null,null,"P=",{"$f":"L12+L13","v":{"$error":"#VALUE!"}},"mmHg",null,null,"Xtoluene=",{"$f":"Q4*Q12/Q8","v":{"$error":"#VALUE!"}},"mol Toluene/ mol",null,null,"nH2O=",{"$f":"V14*V13","v":{"$error":"#VALUE!"}},"kmol H2O/h"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nBDA=",{"$f":"V14*(1-V13)","v":{"$error":"#VALUE!"}},"kmol BDA/h"]
[null,null,null,null,null,null,null,null,null,null,"Ybenzene=",{"$f":"L12/L15","v":{"$error":"#VALUE!"}},"mol Benzene/ mol",null,null,null,null,null,null,null,"nO2=",{"$f":"V16*0.21","v":{"$error":"#VALUE!"}},"kmol O2/h"]
[null,null,null,null,null,null,null,null,null,null,"Ytoluene=",{"$f":"1-L17","v":{"$error":"#VALUE!"}},"mol Toluene/ mol"]
[null,null,null,null,null,null,null,null,null,null,"Example 6.4-3  part 3",null,null,null,null,"Inverse function",null,null,null,null,"(2) Determine the molar humidity, ablsolute humidity, and percentage humidity of the air"]
[null,null,null,null,null,null,null,null,null,null,"Ybenzene=",0.15]
[null,null,null,null,null,null,null,null,null,null,"Ytoluene=",0.1,null,null,null,null,null,null,null,null,"hm=",{"$f":"V11/(W6-V11)","v":{"$error":"#VALUE!"}},"mol H2O/mol BDA"]
[null,null,null,null,null,null,null,null,null,null,"Temperature=",80,"°C",null,null,null,null,null,null,null,"ha=",{"$f":"(V21*18)/29","v":{"$error":"#VALUE!"}},"kg H2O/kg BDA"]
[null,null,null,null,null,null,null,null,null,null,"P*benzene=",{"$f":"[0]!AntoineP(\"Benzene\",L22,\"C\")","v":{"$error":"#VALUE!"}},"mmHg",null,null,{"$f":"[0]!AntoineT(\"benzene\",L23)","v":{"$error":"#VALUE!"}},null,null,null,null,"h*m=",{"$f":"V9/(W6-V9)","v":{"$error":"#VALUE!"}},"kmol H2O/kmol BDA"]
[null,null,null,null,null,null,null,null,null,null,"P*toluene=",{"$f":"[0]!AntoineP(\"Toluene\",L22,\"C\")","v":{"$error":"#VALUE!"}},"mmHg",null,null,{"$f":"[0]!AntoineT(\"toluene\",L24)","v":{"$error":"#VALUE!"}},null,null,null,null,"hp=",{"$f":"100*V21/V23","v":{"$error":"#VALUE!"}},"%"]
[]
[null,null,null,null,null,null,null,null,null,null,"P=",{"$f":"1/((L20/L23)+(L21/L24))","v":{"$error":"#VALUE!"}},"mmHg"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Example: "]
[null,null,null,null,null,null,null,null,null,null,"Xbenzene=",{"$f":"L20*L26/L23","v":{"$error":"#VALUE!"}},"mol Benzene/ mol",null,null,null,null,null,null,null,"1) Find the vapor pressure of water at -13.897°C."]
[null,null,null,null,null,null,null,null,null,null,"Xtoluene=",{"$f":"1-L28","v":{"$error":"#VALUE!"}},"mol Toluene/ mol",null,null,null,null,null,null,null,null,null,"p*H2O(mmHg)=",{"$f":"[0]!VPWater(-13.987,\"c\")","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2) Find the vapor pressure of water at 46.82°C."]
["Problem 6.32",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"p*H2O(mmHg)=",{"$f":"[0]!VPWater(46.82)","v":{"$error":"#VALUE!"}}]
[]
[null,"A gas stream containing 40.0mole% hydrogen, 35.0% carbon monoxide, 20.0% carbon dioxide, and 5.0% methans is cooled from 1000°C to 10°C",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3) Find the vapor pressure of ice at -0.84°C."]
[null,"at a constant absolute pressure of 35.0 atm. Gas enters the cooler at 120 m3/min and upon leaving the cooler is fed to an absorber, where it",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"p*H2O(mmHg)=",{"$f":"[0]!VPWater(-0.84)","v":{"$error":"#VALUE!"}}]
[null,"is contacted with refigerated liquid methanol. The methanol is fed to the absorber at a molar flow rate 1.2 times that of the inlet gas and absorbs "]
[null,"essentially all of the CO2, 98% of the methane, and none of the other components of the feed gas. The gas leaving the absorber, which is saturated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4)Find the vapor pressure of water 51 °C."]
[null,"with methanol at -12°C, is fed to a cross-country pipeline.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"p*H2O(mmHg)=",{"$f":"[0]!VPWater(51)","v":{"$error":"#VALUE!"}}]
[]
[null,"Calculated the volumetric flow rate fo the gas stream entering the absorber (m3/min) and the molar flow rate of methanol in the gas leaving the absorber.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5) What is the boiling point of water at 800 mm Hg?"]
[null,"Do not assume ideal gas behavior when doing PVT calculations.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Using goal seek,"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"p*H2O(mmHg)=",{"$f":"[0]!VPWater(X43)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tb(oC)=",101.44183007837331]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Solution:"]
["Using VBA functions:"]
["Compound","Tc(K)","Pc(atm)","(Tc)corr","(Pc)corr",null,"Corrected values:"]
["H2",{"$f":"[0]!Tcrit(\"hydrogen\")","v":{"$error":"#VALUE!"}},{"$f":"[0]!Pcrit(\"hydrogen\")","v":{"$error":"#VALUE!"}},{"$f":"B65+8","v":{"$error":"#VALUE!"}},{"$f":"C65+8","v":{"$error":"#VALUE!"}},null,null,"eqn(5.4-4)","(Tc)corr = Tc + 8K"]
["CO",{"$f":"[0]!Tcrit(\"carbon monoxide\")","v":{"$error":"#VALUE!"}},{"$f":"[0]!Pcrit(\"carbon monoxide\")","v":{"$error":"#VALUE!"}},"-","-",null,null,"eqn(5.4-5)","(Pc)corr = Pc + 8atm"]
["CO2",{"$f":"[0]!Tcrit(\"carbon dioxide\")","v":{"$error":"#VALUE!"}},{"$f":"[0]!Pcrit(\"carbon dioxide\")","v":{"$error":"#VALUE!"}},"-","-"]
["CH4",{"$f":"[0]!Tcrit(\"methane\")","v":{"$error":"#VALUE!"}},{"$f":"[0]!Pcrit(\"methane\")","v":{"$error":"#VALUE!"}},"-","-"]
[]
[]
["Pseudocritical Values:"]
[null,"eqn (5.4-9)","Tc' = Sum(yiTci)",null,null,null,null,"R=",{"$f":"82.057*10^-3/1000","v":8.2057000000000004E-5},"(m3 atm)/(mol K)"]
[null,null,"Tc' =",{"$f":"0.4*D65+0.35*B66+0.2*B67+0.05*B68","v":{"$error":"#VALUE!"}},"K"]
[null,"eqn (5.4-10)","Pc' = Sum(yiPci)"]
[null,null,"Pc' =",{"$f":"0.4*E65+0.35*C66+0.2*C67+0.05*C68","v":{"$error":"#VALUE!"}},"atm"]
[]
["Cooler inlet:","T=",1000,"C"]
[null,null,{"$f":"+C77+273.15","v":1273.1500000000001},"K",null,null,"eqn (5.4-11)","Tr =",{"$f":"C78/D73","v":{"$error":"#VALUE!"}}]
[null,"P=",35,"atm",null,null,"eqn (5.4-12)","Pr =",{"$f":"C79/D75","v":{"$error":"#VALUE!"}}]
[null,"V=",120,"m3/min",null,null,"Fig(5.4-1) ","zin = ",{"$f":"1.02","v":1.02}]
[null,"eqn (5.4-13) ","Vin =",{"$f":"(I80*I72*C78)/C79","v":3.0445796268857147E-3},"m3/mol"]
[null,null,"nF = ",{"$f":"C80/D81","v":39414.308280958772},"mol/min"]
[]
["Cooler outlet:","T=",10,"C"]
[null,null,{"$f":"+C84+273.15","v":283.14999999999998},"K",null,null,"eqn (5.4-11)","Tr = ",{"$f":"C85/D73","v":{"$error":"#VALUE!"}},"K"]
[null,"P=",35,"atm",null,null,"eqn (5.4-12)","Pr =",{"$f":"C86/D75","v":{"$error":"#VALUE!"}},"atm"]
[null,null,null,null,null,null,"Fig (5.4-3)","zout =",0.98]
[null,"eqn (5.4-13) ","Vout =",{"$f":"(I87*I72*C85)/(C86)","v":6.5056430740000005E-4},"m3/mol"]
[null,null,"VF =",{"$f":"D82*D88","v":25.64154216845203},"m3/min"]
[]
["Raoult's law for methanol:"]
[null,"eqn (6.3-1)","y=p*/P"]
[null,null,"p* =",{"$f":"[0]!AntoineP(\"methanol\",-12,\"c\")","v":{"$error":"#VALUE!"}},"mmHg"]
[null,null,"y1 =",{"$f":"(D93)/(C86*760)","v":{"$error":"#VALUE!"}},"molCH3OH/mol"]
[]
["y1=nmethanol/(ntotal)=nmethanol/(nmethanol+nF*(yH2+0.02*yCH4+yCO)"]
[null,"Solve for f(nmethanol)=0"]
[null,"User solver or goalseek to vary nmethanol until f(nmethanol)=0"]
[null,"f(nmethanol)=",null,{"$f":"D94-D100/(D100+D82*(0.4+0.02*0.05+0.35))","v":{"$error":"#VALUE!"}}]
[null,"nmethanol=",null,14.718840896242341,"mol/min methanol in gas"]

{"sheet":"Chapter 7","index":14,"n_rows":33,"n_cols":23,"rows_kept":33,"cut":false,"hidden":false,"merged":[]}
[null,null,null,null,null,null,null,null,null,"te"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Example 8.3-4  (page 373)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Problem 8.18"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"n (mol/h)=",150]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"nC2H6 =",0.6,null,null,null,null,null,"T1 =",45,"°C"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"nC3H8 =",0.4,null,null,null,null,null,"T2 =",20,"°C"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"T1(°C)=",0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"T2(°C)=",400,null,null,null,null,null,"xa =",0.3,"g acetone/g"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"xm =",0.7,"g 2-methyl-1-pentanol/g"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"∆ĤC2H6 =",{"$f":"[0]!Enthalpy(\"ethane\",O7,O8,\"c\",\"g\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"∆ĤC3H8 =",{"$f":"[0]!Enthalpy(\"propane\",O7,O8,\"C\",\"g\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ĥa for acetone using table B.2"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"∆Ĥmix (kJ/mol)= ",{"$f":"O5*O10+O6*O11","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Ĥa = ",{"$f":"(0.123*(20-45)+18.6*10^-5*0.5*(20-45)^2)/[0]!MW(\"acetone\")","v":{"$error":"#VALUE!"}},"KJ/g"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"V13*1000","v":{"$error":"#VALUE!"}},"J/g"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Q (kJ/h) =",{"$f":"O13*O4","v":{"$error":"#VALUE!"}}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Problem 8.18"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ĥm for 2-methyl-1-pentanol using Kopps rule"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"nC3H6O=",0.3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"nC6H14O=",0.7,null,null,null,null,null,"C",6]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"T1(°C)=",45,null,null,null,null,null,"H",14]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"T2(°C)=",20,null,"For C6H14O Cp estimate",null,null,null,"O",1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Estimated Cp, C6H14O(J/mol C)=",{"$f":"[0]!Kopps(Q25:Q27,R25:R27,\"l\")","v":{"$error":"#VALUE!"}},null,"C",6]
[null,null,null,null,null,null,null,null,null,null,null,null,null," Cp, C6H14O(J/g C)=",{"$f":"+O25/102.17","v":{"$error":"#VALUE!"}},null,"H",14,null,null,"Cpm=",{"$f":"[0]!Kopps(U22:U24,V22:V24,\"L\")/1000","v":{"$error":"#VALUE!"}},"J/(mole °C)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"O",1,null,null,"Cpm=",{"$f":"V26/102","v":{"$error":"#VALUE!"}},"J/(g °C)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Enthalpy changes"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"∆ĤC3H6O(kJ/mol)=",{"$f":"[0]!Enthalpy(\"acetone\",O23,O24,\"C\",\"l\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,"Ĥm =",{"$f":"V27*(V6-V5)","v":{"$error":"#VALUE!"}},"J/g"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"∆ĤC3H6O(kJ/g)=",{"$f":"O29/[0]!MW(\"acetone\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"∆ĤC6H14O(kJ/g)=",{"$f":"O26*(O24-O23)/1000","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"∆H (kJ/g) =",{"$f":"O21*O30+O22*O31","v":{"$error":"#VALUE!"}},null,null,null,null,"ΔH =",{"$f":"0.7*V29+0.3*V14","v":{"$error":"#VALUE!"}},"J/g"]

{"sheet":"Chapter 8","index":15,"n_rows":66,"n_cols":25,"rows_kept":66,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"r","HsHCl","HsNaOH","HmH2SO4"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"inf",{"$f":"[0]!HsHCl(N4)","v":{"$error":"#VALUE!"}},{"$f":"[0]!HsNaOH(N4)","v":{"$error":"#VALUE!"}},{"$f":"[0]!HmH2SO4(N4)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0.5,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,25,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,30,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,500000,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,1000000,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Problem 8.82 "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Use Table B.11 to determine the specific enthalpy (kJ/mol HCl) of hydrochloric acid containing"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"1mol HCl/5mol H2O at 25°C relative to:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"(a) HCl(g) and H2O (l) at 25°C"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"(b) H2O(l) and an infinately dilute HCl solution at 25°C. "]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Solution (a):"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"r = moles of solvent/ moles of solute"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"r =5 mol H2O/mol HCl"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"r =",5]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"ΔĤs = ",{"$f":"[0]!HsHCl(O23)","v":{"$error":"#VALUE!"}},"kJ/mol HCl"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"eqn  (8.5.1)","Ĥ =",{"$f":"1*O25","v":{"$error":"#VALUE!"}},"kJ/mol HCl"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Solution (b):"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"r =",5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"r =","inf"]
["Problem 8.22",null,null,null,null,null,null,null,null,null,null,null,null,"ΔĤs (r=5) = ",{"$f":"[0]!HsHCl(O30)","v":{"$error":"#VALUE!"}},"kJ/mol HCl"]
[null,"A natural gas containing 95 mole% methane and the balance ethane is burned with 25% excess air. The stack",null,null,null,null,null,null,null,null,null,null,null,"ΔĤs (r=inf) = ",{"$f":"[0]!HsHCl(O31)","v":{"$error":"#VALUE!"}},"kJ/mol HCl"]
[null,"gas leaves the furnace at 900°C and 1 atm and contains no unburned hydrocarbons or carbon monoxide. The"]
[null,"gas is cooled to 450°C in a waste heat boiler (a heat exchanger in which heat lost by  cooling gases is used to ",null,null,null,null,null,null,null,null,null,null,null,"Ĥ=",{"$f":"O32-O33","v":{"$error":"#VALUE!"}},"kJ/mol HCl"]
[null,"produce steam from liquid water for heating, power generation, or process applications) prior to being discharged"]
[null,"into the atmosphere. "]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SI version"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Enthalpies relative to 25 °C 1atm, kJ/mol"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T(°C)","Air","Oxygen","Nitrogen","Hydrogen","CO","CO2","water"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,-25,{"$f":"hgassi(\"air\",R47)","v":{"$error":"#VALUE!"}},{"$f":"hgassi(\"o2\",R47)","v":{"$error":"#VALUE!"}},{"$f":"hgassi(\"nitrogen\",R47)","v":{"$error":"#VALUE!"}},{"$f":"hgassi(\"h2\",R47)","v":{"$error":"#VALUE!"}},{"$f":"hgassi(\"Co\",R47)","v":{"$error":"#VALUE!"}},{"$f":"hgassi(\"CO2\",R47)","v":{"$error":"#VALUE!"}},{"$f":"hgassi(\"water\",R47)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Calculate the amount of heat (kJ) that must be transferred from the gas in the boiler to accomplish the indicated cooling. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1400,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Solution:",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1500,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1450,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["References: O2, N2, CO2, H2O (v) at 25°C and 1 atm",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1600,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"nin (mol)","Ĥin(kJ/mol)","nout (mol)","Ĥout(kJ/mol)"]
["O2",51.9,{"$f":"hgassi(\"oxygen\",900)","v":{"$error":"#VALUE!"}},51.9,{"$f":"hgassi(\"oxygen\",450)","v":{"$error":"#VALUE!"}}]
["N2",976,{"$f":"hgassi(\"nitrogen\",900)","v":{"$error":"#VALUE!"}},976,{"$f":"hgassi(\"nitrogen\",450)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,"AES Verison",null,"Enthalpies relative to 77 °F 1atm, BTU/lb-mol"]
["CO2",105,{"$f":"hgassi(\"carbon dioxide\",900)","v":{"$error":"#VALUE!"}},105,{"$f":"hgassi(\"carbon dioxide\",450)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,"T(°F)","Air","Oxygen","Nitrogen","Hydrogen","CO","CO2","water"]
["H2O(v)",205,{"$f":"hgassi(\"water\",900)","v":{"$error":"#VALUE!"}},205,{"$f":"hgassi(\"water\",450)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"hgasAES(\"air\",R59,\"C\")","v":{"$error":"#VALUE!"}},{"$f":"hgasAES(\"o2\",R59)","v":{"$error":"#VALUE!"}},{"$f":"hgasAES(\"nitrogen\",R59)","v":{"$error":"#VALUE!"}},{"$f":"hgasAES(\"h2\",R59)","v":{"$error":"#VALUE!"}},{"$f":"hgasAES(\"Co\",R59)","v":{"$error":"#VALUE!"}},{"$f":"hgasAES(\"CO2\",R59)","v":{"$error":"#VALUE!"}},{"$f":"hgasAES(\"water\",R59)","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,32,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,77,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
["Energy Balance: Q = ΔH = sum(niĤi)out - sum(niĤi)in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,500,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1400,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,"Q=",{"$f":"B56*(E56-C56)+B57*(E57-C57)+B58*(E58-C58)+B59*(E59-C59)","v":{"$error":"#VALUE!"}},"kJ",null,null,null,null,null,null,null,null,null,null,null,null,null,2000,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1950,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2100,{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]

{"sheet":"Chapter 9","index":16,"n_rows":91,"n_cols":18,"rows_kept":91,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,null,null,null,null,null,null,null,null,"Problem 9.55"]
[]
[null,null,null,null,null,null,null,null,null,null,"Methane at 25°C is burned in a boiler furnace with 10.0% excess air preheated to 100°C. Ninety percent of the methane fed is consumed, the product"]
[null,null,null,null,null,null,null,null,null,null,"gass contains 10.0 mol CO2/mol CO, and the combustion products leave the furnace at 400°C."]
[]
[null,null,null,null,null,null,null,null,null,null,"Calculate the heat transferred from the furnace, Q(kW), for a basis of 1000 mol CH4 fed/s.( The great the value of Q, the more steam is produced in the "]
[null,null,null,null,null,null,null,null,null,null,"boiler)"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"CH4 + 2O2 → CO2 + 2H2O",null,null,null,"CH4 + 3/2O2 → CO + 2H2O"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,"Solution:"]
[null,null,null,null,null,null,null,null,null,null,"Oxygen Feed Rate:"]
[null,null,null,null,null,null,null,null,null,null,null,"n0 = 1000 molCH4/s * 2 molO2 required/ mol CH4 * 1.1 molO2 fed/mol O2 required"]
[null,null,null,null,null,null,null,null,null,null,null,"n0 =",{"$f":"1000*2*1.1","v":2200},"mol O2/s"]
[]
[null,null,null,null,null,null,null,null,null,null,"90% methane consumption:"]
["DeltaHfg","Acetone=",{"$f":"[0]!DeltaHfg(\"acetone\")","v":{"$error":"#VALUE!"}},"Methane=",{"$f":"[0]!DeltaHfg(\"methane\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,"n1=(1000 molCH4/fed)(0.1 mol CH4 unconsumed/mol CH4 fed)"]
["DeltaHfl","Acetone=",{"$f":"[0]!DeltaHfl(\"acetone\")","v":{"$error":"#VALUE!"}},"Sulfuric acid=",{"$f":"[0]!DeltaHfl(\"sulfuric acid\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,"n1 =",{"$f":"1000*0.1","v":100},"mol CH3 unconsumed"]
["DeltaHfaq","Acetone=",{"$f":"[0]!DeltaHfaq(\"acetone\")","v":{"$error":"#VALUE!"}},"Sulfuric acid=",{"$f":"[0]!DeltaHfaq(\"sulfuric acid\")","v":{"$error":"#VALUE!"}}]
["DeltaHfc","Acetone=",{"$f":"[0]!DeltaHfc(\"acetone\")","v":{"$error":"#VALUE!"}},"sodium hydroxide=",{"$f":"[0]!DeltaHfc(\"sodium hydroxide\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,"C balance:"]
["DeltaHcg","Acetone=",{"$f":"[0]!DeltaHcg(\"acetone\")","v":{"$error":"#VALUE!"}},"m-Xylene=",{"$f":"[0]!DeltaHcg(\"m-xylene\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,"1000 molCH4/s(1molCO/1molCH4) = 1n1 + 1n3 + 10n3"]
["DeltaHcl","Acetone=",{"$f":"[0]!DeltaHcl(\"acetone\")","v":{"$error":"#VALUE!"}},"m-Xylene=",{"$f":"[0]!DeltaHcl(\"m-xylene\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,"1000 molC = 1n1 + 11n3"]
["DeltaHcc","Acetone=",{"$f":"[0]!DeltaHcc(\"acetone\")","v":{"$error":"#VALUE!"}},"Carbon (Graphite)=",{"$f":"[0]!DeltaHcc(\"carbon (graphite)\")","v":{"$error":"#VALUE!"}}]
["DeltaHcs","Acetone=",{"$f":"[0]!DeltaHcs(\"acetone\")","v":{"$error":"#VALUE!"}},"Phenol=",{"$f":"[0]!DeltaHcs(\"phenol\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,"H balance:"]
[null,null,null,null,null,null,null,null,null,null,null,"1000molCH4/s (4molH/1molCH4) = 4n1 + 2n4"]
["Example 9.4-1 (p. 449):"]
["Calculate the standard heat of reaction for the dehydrogentaion of ethane:",null,null,null,null,null,null,null,null,null,"O balance:"]
[null,"C6H6→C2H4 + H2",null,null,null,null,null,null,null,null,null,"2n0 = 2n2 + 1n3 + 2(10)n3 + 1n4"]
[null,null,null,null,null,null,null,null,null,null,null,"2n0 = 2n2 + 21n3 + 1n4"]
["Solution:"]
["Using VBA functions:","(ΔĤc°)C2H6=",{"$f":"[0]!DeltaHcg(\"ethane\")","v":{"$error":"#VALUE!"}},"kJ/mol",null,null,null,null,null,"References: C(s), H2(g),O2(g),N2(g) @ 25°C, 1 atm"]
[null,"(ΔĤc°)C2H4=",{"$f":"[0]!DeltaHcg(\"ethylene\")","v":{"$error":"#VALUE!"}},"kJ/mol",null,null,null,null,null,null,"nin(mol/s)","Ĥin(kJ/mol)","nout(mol/s)","Ĥout(kJ/mol)"]
[null,"(ΔĤc°)H2=",{"$f":"[0]!DeltaHcg(\"hydrogen\")","v":{"$error":"#VALUE!"}},"kJ/mol",null,null,null,null,null,"CH4(g)",1000,"ĤA","n1","ĤD"]
[null,null,null,null,null,null,null,null,null,"O2(g)","n0","ĤB","n2","ĤE"]
["eqn (9.4-1):","ΔĤr°=(ΔĤc°)C2H6 -(ΔĤc°)C2H4 -(ΔĤc°)H2",null,null,null,null,null,null,null,"N2(g)","3.76n0","ĤC","3.76n0","ĤF"]
[null,null,null,null,null,null,null,null,null,"CO(g)","-","-","n3","ĤG"]
[null,"ΔĤr°=",{"$f":"C49-C50-C51","v":{"$error":"#VALUE!"}},"kJ/mol",null,null,null,null,null,"CO2(g)","-","-","10n3","ĤH"]
[null,null,null,null,null,null,null,null,null,"H2O(v)","-","-","n4","ĤI"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"UsingAdd-In Functions:  "]
[null,null,null,null,null,null,null,null,null,null,null,"ĤA=",{"$f":"[0]!DeltaHfg(\"methane\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,"ĤB=",{"$f":"[0]!Enthalpy(\"oxygen\",25,100,\"c\",\"g\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,"ĤC=",{"$f":"[0]!Enthalpy(\"nitrogen\",25,100,\"c\",\"g\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,"ĤD=",{"$f":"[0]!DeltaHfg(\"methane\")+[0]!Enthalpy(\"methane\",25,400,\"c\",\"g\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,"ĤE=",{"$f":"[0]!Enthalpy(\"oxygen\",25,400,\"c\",\"g\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,"ĤF=",{"$f":"[0]!Enthalpy(\"nitrogen\",25,400,\"c\",\"g\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,"ĤG=",{"$f":"[0]!DeltaHfg(\"carbon monoxide\")+[0]!Enthalpy(\"carbon monoxide\",25,400,\"c\",\"g\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,"ĤH=",{"$f":"[0]!DeltaHfg(\"carbon dioxide\")+[0]!Enthalpy(\"carbon dioxide\",25,400,\"c\",\"g\")","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,null,null,null,null,"ĤI=",{"$f":"[0]!DeltaHfg(\"water\")+[0]!Enthalpy(\"water\",25,400,\"c\",\"g\")","v":{"$error":"#VALUE!"}}]
[]
[null,null,null,null,null,null,null,null,null,null,"Energy balance:"]
[null,null,null,null,null,null,null,null,null,null,null,"Q = Sum(niĤi)out - Sum(niĤi)out"]
[null,null,null,null,null,null,null,null,null,null,null,"Q = n1ĤD + n2ĤE + 3.76n0ĤF + n3ĤG + 10n3ĤH + n4ĤI - 1000ĤA - n0ĤB - 3.76n0Ĥc"]
[]
[null,null,null,null,null,null,null,null,null,"Solve using matrix methods:"]
[]
[null,null,null,null,null,null,null,null,null,"Atomic Balances:",null,"1000 - n1 = 0n2 + 11n3 + 0n4"]
[null,null,null,null,null,null,null,null,null,null,null,"4000 - 4n1 = 0n2 + 0n3 + 2n4"]
[null,null,null,null,null,null,null,null,null,null,null,"2n0 - 0n1 = 2n2 + 21n3 + 1n4"]
[]
[null,null,null,null,null,null,null,null,null,null,0,11,0,null,{"$f":"1000-M36","v":900},null,"n2 =",{"$f":"MMULT(MINVERSE(K80:M82),O80:O82)","v":440.90909090909099}]
[null,null,null,null,null,null,null,null,null,null,0,0,2,null,{"$f":"4000-4*M36","v":3600},null,"n3 =",81.818181818181827]
[null,null,null,null,null,null,null,null,null,null,2,21,1,null,{"$f":"2*M32","v":4400},null,"n4 =",1800]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"n0 =",{"$f":"M32","v":2200}]
[null,null,null,null,null,null,null,null,null,null,null,null,"n1 =",{"$f":"M36","v":100}]
[null,null,null,null,null,null,null,null,null,null,null,null,"n2 =",{"$f":"R80","v":440.90909090909099}]
[null,null,null,null,null,null,null,null,null,null,null,null,"n3 =",{"$f":"R81","v":81.818181818181827}]
[null,null,null,null,null,null,null,null,null,null,null,null,"n4 =",{"$f":"R82","v":1800}]
[null,null,null,null,null,null,null,null,null,"Answer:"]
[null,null,null,null,null,null,null,null,null,null,"Q = ",{"$f":"N85*M63+N86*M64+3.76*N84*M65+N87*M66+10*N87*M67+N88*M68-1000*M60-N84*M61-3.76*N84*M62","v":{"$error":"#VALUE!"}},"kW"]
[null,null,null,null,null,null,null,null,null,null,"Q = ",{"$f":"L90","v":{"$error":"#VALUE!"}},"kW"]

{"sheet":"Chapter 10","index":17,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Chapter 11","index":18,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"B6","index":19,"n_rows":173,"n_cols":9,"rows_kept":173,"cut":false,"hidden":true,"merged":[]}
["Properties of Saturated Steam: Pressure Table"]
[null,null,"V (m^3/kg)","V (m^3/kg)","U (kJ/kg)","U (kJ/kg)","H (kJ/kg)","H (kJ/kg)","H (kJ/kg)"]
["P(bar)","T(°C)","Water","Steam","Water","Steam","Water","Evaporation","Steam"]
[6.11E-3,0.01,1E-3,206.2,"zero",2375.6,0,2501.6,2501.6]
[8.0000000000000002E-3,3.8,1E-3,159.69999999999999,15.8,2380.6999999999998,15.8,2492.6,2508.5]
[0.01,7,1E-3,129.19999999999999,29.3,2385.1999999999998,29.3,2485,2514.4]
[1.2E-2,9.6999999999999993,1E-3,108.7,40.6,2388.9,40.6,2478.6999999999998,2519.3000000000002]
[1.4E-2,12,1E-3,93.9,50.3,2392,50.3,2473.1999999999998,2523.5]
[1.6E-2,14,1.0009999999999999E-3,82.8,58.9,2394.8000000000002,58.9,2468.4,2527.3000000000002]
[1.7999999999999999E-2,15.9,1.0009999999999999E-3,74,66.5,2397.4,66.5,2464.1,2530.6]
[0.02,17.5,1.0009999999999999E-3,67,73.5,2399.6,73.5,2460.1999999999998,2533.6]
[2.1999999999999999E-2,19,1.0020000000000001E-3,61.2,79.8,2401.6999999999998,79.8,2456.6,2536.4]
[2.4E-2,20.399999999999999,1.0020000000000001E-3,56.4,85.7,2403.6,85.7,2453.3000000000002,2539]
[2.5999999999999999E-2,21.7,1.0020000000000001E-3,52.3,91.1,2405.4,91.1,2450.1999999999998,2541.3000000000002]
[2.8000000000000001E-2,23,1.0020000000000001E-3,48.7,96.2,2407.1,96.2,2447.3000000000002,2543.6]
[0.03,24.1,1.003E-3,45.7,101,2408.6,101,2444.6,2545.6]
[3.5000000000000003E-2,26.7,1.003E-3,39.5,111.8,2412.1999999999998,111.8,2438.5,2550.4]
[0.04,29,1.0039999999999999E-3,34.799999999999997,121.4,2415.3000000000002,121.4,2433.1,2554.5]
[4.4999999999999998E-2,31,1.005E-3,31.1,130,2418.1,130,2428.1999999999998,2558.1999999999998]
[0.05,32.9,1.005E-3,28.2,137.80000000000001,2420.6,137.80000000000001,2423.8000000000002,2561.6]
[0.06,36.200000000000003,1.0059999999999999E-3,23.74,151.5,2425.1,151.5,2416,2567.5]
[7.0000000000000007E-2,39,1.0070000000000001E-3,20.53,163.4,2428.9,163.4,2409.1999999999998,2572.6]
[0.08,41.5,1.008E-3,18.100000000000001,173.9,2432.3000000000002,173.9,2403.1999999999998,2577.1]
[0.09,43.8,1.0089999999999999E-3,16.2,183.3,2435.3000000000002,183.3,2397.9,2581.1]
[0.1,45.8,1.01E-3,14.67,191.8,2438,191.8,2392.9,2584.8000000000002]
[0.11,47.7,1.011E-3,13.42,199.7,2440.5,199.7,2388.4,2588.1]
[0.12,49.4,1.0120000000000001E-3,12.36,206.9,2442.8000000000002,206.9,2384.3000000000002,2591.1999999999998]
[0.13,51.1,1.013E-3,11.47,213.7,2445,213.7,2380.4,2594]
[0.14000000000000001,52.6,1.013E-3,10.69,220,2447,220,2376.6999999999998,2596.6999999999998]
[0.15,54,1.0139999999999999E-3,10.02,226,2448.9,226,2373.1999999999998,2599.1999999999998]
[0.16,55.3,1.0150000000000001E-3,9.43,231.6,2450.6,231.6,2370,2601.6]
[0.17,56.6,1.0150000000000001E-3,8.91,236.9,2452.3000000000002,236.9,2366.9,2603.8000000000002]
[0.18,57.8,1.016E-3,8.4499999999999993,242,2453.9,242,2363.9,2605.9]
[0.19,59,1.0169999999999999E-3,8.0299999999999994,246.8,2455.4,246.8,2361.1,2607.9]
[0.2,60.1,1.0169999999999999E-3,7.65,251.5,2456.9,251.5,2358.4,2609.9]
[0.22,62.2,1.018E-3,7,260.10000000000002,2459.6,260.10000000000002,2353.3000000000002,2613.5]
[0.24,64.099999999999994,1.0189999999999999E-3,6.45,268.2,2462.1,268.2,2348.6,2616.8000000000002]
[0.26,65.900000000000006,1.0200000000000001E-3,5.98,275.60000000000002,2464.4,275.7,2344.1999999999998,2619.9]
[0.28000000000000003,67.5,1.021E-3,5.58,282.7,2466.5,282.7,2340,2622.7]
[0.3,69.099999999999994,1.0219999999999999E-3,5.23,289.3,2468.6,289.3,2336.1,2625.4]
[0.35,72.7,1.0250000000000001E-3,4.53,304.3,2473.1,304.3,2327.1999999999998,2631.5]
[0.4,75.900000000000006,1.0269999999999999E-3,3.99,317.60000000000002,2477.1,317.7,2319.1999999999998,2636.9]
[0.45,78.7,1.0280000000000001E-3,3.58,329.6,2480.6999999999998,329.6,2312,2641.7]
[0.5,81.3,1.0300000000000001E-3,3.24,340.5,2484,340.6,2305.4,2646]
[0.55000000000000004,83.7,1.0319999999999999E-3,2.96,350.6,2486.9,350.6,2299.3000000000002,2649.9]
[0.6,86,1.0330000000000001E-3,2.73,359.9,2489.6999999999998,359.9,2293.6,2653.6]
[0.65,88,1.0349999999999999E-3,2.5299999999999998,368.5,2492.1999999999998,368.6,2288.3000000000002,2656.9]
[0.7,90,1.036E-3,2.36,376.7,2494.5,376.8,2283.3000000000002,2660.1]
[0.75,91.8,1.0369999999999999E-3,2.2200000000000002,384.4,2496.6999999999998,384.5,2278.6,2663]
[0.8,93.5,1.039E-3,2.0870000000000002,391.6,2498.8000000000002,391.7,2274.1,2665.8]
[0.85,95.2,1.0399999999999999E-3,1.972,398.5,2500.8000000000002,398.6,2269.8000000000002,2668.4]
[0.9,96.7,1.041E-3,1.869,405.1,2502.6,405.2,2265.6,2670.9]
[0.95,98.2,1.042E-3,1.7769999999999999,411.4,2504.4,411.5,2261.6999999999998,2673.2]
[1,99.6,1.0430000000000001E-3,1.694,417.4,2506.1,417.5,2257.9,2675.4]
[1.01325,100,1.044E-3,1.673,419,2506.5,419.1,2256.9,2676]
[1.1000000000000001,102.3,1.0460000000000001E-3,1.5489999999999999,428.7,2509.1999999999998,428.8,2250.8000000000002,2679.6]
[1.2,104.8,1.0480000000000001E-3,1.4279999999999999,439.2,2512.1,439.4,2244.1,2683.4]
[1.3,107.1,1.049E-3,1.325,449.1,2514.6999999999998,449.2,2237.8000000000002,2687]
[1.4,109.3,1.0510000000000001E-3,1.236,458.3,2517.1999999999998,458.4,2231.9,2690.3]
[1.5,111.4,1.0529999999999999E-3,1.159,467,2519.5,467.1,2226.1999999999998,2693.4]
[1.6,113.3,1.0549999999999999E-3,1.091,475.2,2521.6999999999998,475.4,2220.9,2696.2]
[1.7,115.2,1.0560000000000001E-3,1.0309999999999999,483,2523.6999999999998,483.2,2215.6999999999998,2699]
[1.8,116.9,1.0579999999999999E-3,0.97699999999999998,490.5,2525.6,490.7,2210.8000000000002,2701.5]
[1.9,118.6,1.059E-3,0.92900000000000005,497.6,2527.5,497.8,2206.1,2704]
[2,120.2,1.0610000000000001E-3,0.88500000000000001,504.5,2529.1999999999998,504.7,2201.6,2706.3]
[2.2000000000000002,123.3,1.0640000000000001E-3,0.81,517.4,2532.4,517.6,2193,2710.6]
[2.4,126.1,1.0660000000000001E-3,0.746,529.4,2535.4,529.6,2184.9,2714.5]
[2.6,128.69999999999999,1.0690000000000001E-3,0.69299999999999995,540.6,2538.1,540.9,2177.3000000000002,2718.2]
[2.8,131.19999999999999,1.0709999999999999E-3,0.64600000000000002,551.1,2540.6,551.4,2170.1,2721.5]
[3,133.5,1.0740000000000001E-3,0.60599999999999998,561.1,2543,561.4,2163.1999999999998,2724.7]
[3.2,135.80000000000001,1.0759999999999999E-3,0.56999999999999995,570.6,2545.1999999999998,570.9,2156.6999999999998,2727.6]
[3.4,137.9,1.078E-3,0.53800000000000003,579.6,2547.1999999999998,579.9,2150.4,2730.3]
[3.6,139.9,1.08E-3,0.51,588.1,2549.1999999999998,588.5,2144.4,2732.9]
[3.8,141.80000000000001,1.0820000000000001E-3,0.48499999999999999,596.4,2551,596.79999999999995,2138.6,2735.3]
[4,143.6,1.0839999999999999E-3,0.46200000000000002,604.20000000000005,2552.6999999999998,604.70000000000005,2133,2737.6]
[4.2,145.4,1.0859999999999999E-3,0.442,611.79999999999995,2554.4,612.29999999999995,2127.5,2739.8]
[4.4000000000000004,147.1,1.088E-3,0.42299999999999999,619.1,2555.9,619.6,2122.3000000000002,2741.9]
[4.5999999999999996,148.69999999999999,1.0889999999999999E-3,0.40500000000000003,626.20000000000005,2557.4,626.70000000000005,2117.1999999999998,2743.9]
[4.8,150.30000000000001,1.091E-3,0.38900000000000001,633,2558.8000000000002,633.5,2112.1999999999998,2745.7]
[5,151.80000000000001,1.093E-3,0.375,639.6,2560.1999999999998,640.1,2107.4,2747.5]
[5.5,155.5,1.0970000000000001E-3,0.34200000000000003,655.20000000000005,2563.3000000000002,655.8,2095.9,2751.7]
[6,158.80000000000001,1.101E-3,0.315,669.8,2566.1999999999998,670.4,2085,2755.5]
[6.5,162,1.1050000000000001E-3,0.29199999999999998,683.4,2568.6999999999998,684.1,2074.6999999999998,2758.9]
[7,165,1.108E-3,0.27300000000000002,696.3,2571.1,697.1,2064.9,2762]
[7.5,167.8,1.1119999999999999E-3,0.25540000000000002,708.5,2573.3000000000002,709.3,2055.5,2764.8]
[8,170.4,1.1150000000000001E-3,0.24030000000000001,720,2575.5,720.9,2046.5,2767.5]
[8.5,172.9,1.1180000000000001E-3,0.2268,731.1,2577.1,732,2037.9,2769.9]
[9,175.4,1.121E-3,0.21479999999999999,741.6,2578.8000000000002,742.6,2029.5,2772.1]
[9.5,177.7,1.124E-3,0.20399999999999999,751.8,2580.4,752.8,2021.4,2774.2]
[10,179.9,1.127E-3,0.1943,761.5,2581.9,762.6,2013.6,2776.2]
[10.5,182,1.1299999999999999E-3,0.1855,770.8,2583.3000000000002,772,2005.9,2778]
[11,184.1,1.1329999999999999E-3,0.1774,779.9,2584.5,781.1,1998.5,2779.7]
[11.5,186,1.1360000000000001E-3,0.17,788.6,2585.8000000000002,789.9,1991.3,2781.3]
[12,188,1.139E-3,0.16320000000000001,797.1,2586.9,798.4,1984.3,2782.7]
[12.5,189.8,1.1410000000000001E-3,0.15690000000000001,805.3,2588,806.7,1977.4,2784.1]
[13,191.6,1.1440000000000001E-3,0.15110000000000001,813.2,2589,814.7,1970.7,2785.4]
[14,195,1.1490000000000001E-3,0.14069999999999999,828.5,2590.8000000000002,830.1,1957.7,2787.8]
[15,198.3,1.1540000000000001E-3,0.13170000000000001,842.9,2592.4,844.7,1945.2,2789.9]
[16,201.4,1.1590000000000001E-3,0.1237,856.7,2593.8000000000002,858.6,1933.2,2791.7]
[17,204.3,1.163E-3,0.1166,869.9,2595.1,871.8,1921.5,2793.4]
[18,207.1,1.168E-3,0.1103,882.5,2596.3000000000002,884.6,1910.3,2794.8]
[19,209.8,1.1720000000000001E-3,0.1047,894.6,2597.3000000000002,896.8,1899.3,2796.1]
[20,212.4,1.1770000000000001E-3,9.9500000000000005E-2,906.2,2598.1999999999998,908.6,1888.6,2797.2]
[21,214.9,1.181E-3,9.4899999999999998E-2,917.5,2598.9,920,1878.2,2798.2]
[22,217.2,1.1850000000000001E-3,9.0700000000000003E-2,928.3,2599.6,931,1868.1,2799.1]
[23,219.6,1.189E-3,8.6800000000000002E-2,938.9,2600.1999999999998,941.6,1858.2,2799.8]
[24,221.8,1.193E-3,8.3199999999999996E-2,949.1,2600.6999999999998,951.9,1848.5,2800.4]
[25,223.9,1.1969999999999999E-3,7.9899999999999999E-2,959,2601.1999999999998,962,1839,2800.9]
[26,226,1.201E-3,7.6899999999999996E-2,968.6,2601.5,971.7,1829.6,2801.4]
[27,228.1,1.2049999999999999E-3,7.3999999999999996E-2,978,2601.8000000000002,981.2,1820.5,2801.7]
[28,230,1.209E-3,7.1400000000000005E-2,987.1,2602.1,990.5,1811.5,2802]
[29,232,1.2130000000000001E-3,6.8900000000000003E-2,996,2602.3000000000002,999.5,1802.6,2802.2]
[30,233.8,1.2160000000000001E-3,6.6600000000000006E-2,1004.7,2602.4,1008.4,1793.9,2802.3]
[32,237.4,1.224E-3,6.2399999999999997E-2,1021.5,2602.5,1025.4000000000001,1776.9,2802.3]
[34,240.9,1.2310000000000001E-3,5.8700000000000002E-2,1037.5999999999999,2602.5,1041.8,1760.3,2802.1]
[36,244.2,1.238E-3,5.5399999999999998E-2,1053.0999999999999,2602.1999999999998,1057.5999999999999,1744.2,2801.7]
[38,247.3,1.245E-3,5.2400000000000002E-2,1068,2601.9,1072.7,1728.4,2801.1]
[40,250.3,1.2520000000000001E-3,4.9700000000000001E-2,1082.4000000000001,2601.3000000000002,1087.4000000000001,1712.9,2800.3]
[42,253.2,1.2589999999999999E-3,4.7300000000000002E-2,1096.3,2600.6999999999998,1101.5999999999999,1697.8,2799.4]
[44,256,1.266E-3,4.5100000000000001E-2,1109.8,2599.9,1115.4000000000001,1682.9,2798.3]
[46,258.8,1.2719999999999999E-3,4.2999999999999997E-2,1122.9000000000001,2599.1,1128.8,1668.3,2797.1]
[48,261.39999999999998,1.279E-3,4.1200000000000001E-2,1135.5999999999999,2598.1,1141.8,1653.9,2795.7]
[50,263.89999999999998,1.286E-3,3.9399999999999998E-2,1148,2597,1154.5,1639.7,2794.2]
[52,266.39999999999998,1.292E-3,3.78E-2,1160.0999999999999,2595.9,1166.8,1625.7,2792.6]
[54,268.8,1.299E-3,3.6299999999999999E-2,1171.9000000000001,2594.6,1178.9000000000001,1611.9,2790.8]
[56,271.10000000000002,1.3060000000000001E-3,3.49E-2,1183.5,2593.3000000000002,1190.8,1598.2,2789]
[58,273.3,1.312E-3,3.3700000000000001E-2,1194.7,2591.9,1202.3,1584.7,2787]
[60,275.60000000000002,1.3190000000000001E-3,3.2399999999999998E-2,1205.8,2590.4,1213.7,1571.3,2785]
[62,277.7,1.325E-3,3.1300000000000001E-2,1216.5999999999999,2588.8000000000002,1224.8,1558,2782.9]
[64,279.8,1.3320000000000001E-3,3.0200000000000001E-2,1227.2,2587.1999999999998,1235.7,1544.9,2780.6]
[66,281.8,1.338E-3,2.92E-2,1237.5999999999999,2585.5,1246.5,1531.9,2778.3]
[68,283.8,1.3450000000000001E-3,2.8299999999999999E-2,1247.9000000000001,2583.6999999999998,1257,1518.9,2775.9]
[70,285.8,1.351E-3,2.7400000000000001E-2,1258,2581.8000000000002,1267.4000000000001,1506,2773.5]
[72,287.7,1.358E-3,2.6499999999999999E-2,1267.9000000000001,2579.9,1277.5999999999999,1493.3,2770.9]
[74,289.60000000000002,1.364E-3,2.5700000000000001E-2,1277.5999999999999,2578,1287.7,1480.5,2768.3]
[76,291.39999999999998,1.371E-3,2.4899999999999999E-2,1287.2,2575.9,1297.5999999999999,1467.9,2765.5]
[78,293.2,1.3780000000000001E-3,2.4199999999999999E-2,1296.7,2573.8000000000002,1307.4000000000001,1455.3,2762.8]
[80,295,1.384E-3,2.35E-2,1306,2571.6999999999998,1317.1,1442.8,2759.9]
[82,296.7,1.3910000000000001E-3,2.29E-2,1315.2,2569.5,1326.6,1430.3,2757]
[84,298.39999999999998,1.3979999999999999E-3,2.2200000000000001E-2,1324.3,2567.1999999999998,1336.1,1417.9,2754]
[86,300.10000000000002,1.4040000000000001E-3,2.1600000000000001E-2,1333.3,2564.9,1345.4,1405.5,2750.9]
[88,301.7,1.4109999999999999E-3,2.1000000000000001E-2,1342.2,2562.6,1354.6,1393.2,2747.8]
[90,303.3,1.418E-3,2.0500000000000001E-2,1351,2560.1,1363.7,1380.9,2744.6]
[92,304.89999999999998,1.4250000000000001E-3,1.9959999999999999E-2,1359.7,2557.6999999999998,1372.8,1368.6,2741.4]
[94,306.39999999999998,1.4319999999999999E-3,1.9449999999999999E-2,1368.2,2555.1999999999998,1381.7,1356.3,2738]
[96,308,1.439E-3,1.8970000000000001E-2,1376.7,2552.6,1390.6,1344.1,2734.7]
[98,309.5,1.446E-3,1.8489999999999999E-2,1385.2,2550,1399.3,1331.9,2731.2]
[100,311,1.4530000000000001E-3,1.804E-2,1393.5,2547.3000000000002,1408,1319.7,2727.7]
[105,314.60000000000002,1.47E-3,1.6979999999999999E-2,1414.1,2540.4,1429.5,1289.2,2718.7]
[110,318,1.4890000000000001E-3,1.601E-2,1434.2,2533.1999999999998,1450.6,1258.7,2709.3]
[115,321.39999999999998,1.5070000000000001E-3,1.511E-2,1454,2525.6999999999998,1471.3,1228.2,2699.5]
[120,324.60000000000002,1.5269999999999999E-3,1.4279999999999999E-2,1473.4,2517.8000000000002,1491.8,1197.4000000000001,2689.2]
[125,327.8,1.547E-3,1.3509999999999999E-2,1492.7,2509.4,1512,1166.4000000000001,2678.4]
[130,330.8,1.567E-3,1.2800000000000001E-2,1511.6,2500.6,1532,1135,2667]
[135,333.8,1.588E-3,1.213E-2,1530.4,2491.3000000000002,1551.9,1103.0999999999999,2655]
[140,336.6,1.611E-3,1.15E-2,1549.1,2481.4,1571.6,1070.7,2642.4]
[145,339.4,1.634E-3,1.09E-2,1567.5,2471,1591.3,1037.7,2629.1]
[150,342.1,1.658E-3,1.034E-2,1586.1,2459.9,1611,1004,2615]
[155,344.8,1.683E-3,9.8099999999999993E-3,1604.6,2448.1999999999998,1630.7,969.6,2600.3000000000002]
[160,347.3,1.7099999999999999E-3,9.3100000000000006E-3,1623.2,2436,1650.5,934.3,2584.9]
[165,349.8,1.7390000000000001E-3,8.8299999999999993E-3,1641.8,2423.1,1670.5,898.3,2568.8000000000002]
[170,352.3,1.7700000000000001E-3,8.3700000000000007E-3,1661.6,2409.3000000000002,1691.7,859.9,2551.6]
[175,354.6,1.8029999999999999E-3,7.9299999999999995E-3,1681.8,2394.6,1713.3,820,2533.3000000000002]
[180,357,1.8400000000000001E-3,7.4999999999999997E-3,1701.7,2378.9,1734.8,779.1,2513.9]
[185,359.2,1.8810000000000001E-3,7.0800000000000004E-3,1721.7,2362.1,1756.5,736.6,2493.1]
[190,361.4,1.926E-3,6.6800000000000002E-3,1742.1,2343.8000000000002,1778.7,692,2470.6]
[195,363.6,1.977E-3,6.28E-3,1763.2,2323.6,1801.8,644.20000000000005,2446]
[200,365.7,2.0400000000000001E-3,5.8799999999999998E-3,1785.7,2300.8000000000002,1826.5,591.9,2418.4]
[205,367.8,2.1099999999999999E-3,5.4599999999999996E-3,1810.7,2274.4,1853.9,532.5,2386.4]
[210,369.8,2.2000000000000001E-3,5.0200000000000002E-3,1840,2242.1,1886.3,461.3,2347.6]
[215,371.8,2.3400000000000001E-3,4.5100000000000001E-3,1878.6,2198.1,1928.9,366.2,2295.1999999999998]
[220,373.7,2.6700000000000001E-3,3.7299999999999998E-3,1952,2114,2011,185,2196]
[221.2,374.15,3.1700000000000001E-3,3.1700000000000001E-3,2038,2038,2108,0,2108]

{"sheet":"B5","index":20,"n_rows":55,"n_cols":9,"rows_kept":55,"cut":false,"hidden":true,"merged":[]}
[null,null,"V(m3/kg)","V(m3/kg)","U(kJ/kg)","U(kJ/kg)","H(kJ/kg)","H(kJ/kg)","H(kJ/kg)"]
["T(°C)","P(bar)","Water","Steam","Water","Steam","Water","Evaporation","Steam"]
[0.01,6.11E-3,1E-3,206.2,"zero",2375.6,0,2501.6,2501.6]
[2,7.0499999999999998E-3,1E-3,179.9,8.4,2378.3000000000002,8.4,2496.8000000000002,2505.1999999999998]
[4,8.1300000000000001E-3,1E-3,157.30000000000001,16.8,2381.1,16.8,2492.1,2508.9]
[6,9.3500000000000007E-3,1E-3,137.80000000000001,25.2,2383.8000000000002,25.2,2487.4,2512.6]
[8,1.072E-2,1E-3,121,33.6,2386.6,33.6,2482.6,2516.1999999999998]
[10,1.227E-2,1E-3,106.4,42,2389.3000000000002,42,2477.9,2519.9]
[12,1.401E-2,1E-3,93.8,50.4,2392.1,50.4,2473.1999999999998,2523.6]
[14,1.5970000000000002E-2,1.0009999999999999E-3,82.9,58.8,2394.8000000000002,58.8,2468.5,2527.1999999999998]
[16,1.8169999999999999E-2,1.0009999999999999E-3,73.400000000000006,67.099999999999994,2397.6,67.099999999999994,2463.8000000000002,2530.9]
[18,2.0619999999999999E-2,1.0009999999999999E-3,65.099999999999994,75.5,2400.3000000000002,75.5,2459,2534.5]
[20,2.3400000000000001E-2,1.0020000000000001E-3,57.8,83.9,2403,83.9,2454.3000000000002,2538.1999999999998]
[22,2.64E-2,1.0020000000000001E-3,51.5,92.2,2405.8000000000002,92.2,2449.6,2541.8000000000002]
[24,2.98E-2,1.003E-3,45.9,100.6,2408.5,100.6,2444.9,2545.5]
[25,3.1699999999999999E-2,1.003E-3,43.4,104.8,2409.9,104.8,2442.5,2547.3000000000002]
[26,3.3599999999999998E-2,1.003E-3,41,108.9,2411.1999999999998,108.9,2440.1999999999998,2549.1]
[28,3.78E-2,1.0039999999999999E-3,36.700000000000003,117.3,2414,117.3,2435.4,2552.6999999999998]
[30,4.24E-2,1.0039999999999999E-3,32.9,125.7,2416.6999999999998,125.7,2430.6999999999998,2556.4]
[32,4.7500000000000001E-2,1.005E-3,29.6,134,2419.4,134,2425.9,2560]
[34,5.3199999999999997E-2,1.0059999999999999E-3,26.6,142.4,2422.1,142.4,2421.1999999999998,2563.6]
[36,5.9400000000000001E-2,1.0059999999999999E-3,24,150.69999999999999,2424.8000000000002,150.69999999999999,2416.4,2567.1999999999998]
[38,6.6199999999999995E-2,1.0070000000000001E-3,21.6,159.1,2427.5,159.1,2411.6999999999998,2570.8000000000002]
[40,7.3800000000000004E-2,1.008E-3,19.55,167.4,2430.1999999999998,167.5,2406.9,2574.4]
[42,8.2000000000000003E-2,1.0089999999999999E-3,17.690000000000001,175.8,2432.9,175.8,2402.1,2577.9]
[44,9.0999999999999998E-2,1.0089999999999999E-3,16.04,184.2,2435.6,184.2,2397.3000000000002,2581.5]
[46,0.1009,1.01E-3,14.56,192.5,2438.3000000000002,192.5,2392.5,2585.1]
[48,0.1116,1.011E-3,13.23,200.9,2440.9,200.9,2387.6999999999998,2588.6]
[50,0.1234,1.0120000000000001E-3,12.05,209.2,2443.6,209.3,2382.9,2592.1999999999998]
[52,0.1361,1.013E-3,10.98,217.7,2446,217.7,2377,2595]
[54,0.15,1.0139999999999999E-3,10.02,226,2449,226,2373,2599]
[56,0.1651,1.0150000000000001E-3,9.1579999999999995,234.4,2451,234.4,2368,2602]
[58,0.18149999999999999,1.016E-3,8.3800000000000008,242.8,2454,242.8,2363,2606]
[60,0.19919999999999999,1.0169999999999999E-3,7.6779999999999999,251.1,2456,251.1,2358,2609]
[62,0.21840000000000001,1.018E-3,7.0430000000000001,259.5,2459,259.5,2353,2613]
[64,0.23910000000000001,1.0189999999999999E-3,6.468,267.89999999999998,2461,267.89999999999998,2348,2616]
[66,0.26150000000000001,1.0200000000000001E-3,5.9470000000000001,276.2,2464,276.2,2343,2619]
[68,0.28560000000000002,1.0219999999999999E-3,5.4749999999999996,284.60000000000002,2467,284.60000000000002,2338,2623]
[70,0.31169999999999998,1.023E-3,5.0449999999999999,293,2469,293,2333,2626]
[72,0.33960000000000001,1.024E-3,4.6550000000000002,301.39999999999998,2472,301.39999999999998,2329,2630]
[74,0.36959999999999998,1.0250000000000001E-3,4.2990000000000004,309.8,2474,309.8,2323,2633]
[76,0.40189999999999998,1.026E-3,3.9750000000000001,318.2,2476,318.2,2318,2636]
[78,0.4365,1.0280000000000001E-3,3.6789999999999998,326.39999999999998,2479,326.39999999999998,2313,2639]
[80,0.47360000000000002,1.029E-3,3.4079999999999999,334.8,2482,334.9,2308,2643]
[82,0.51329999999999998,1.0300000000000001E-3,3.161,343.2,2484,343.3,2303,2646]
[84,0.55579999999999996,1.0319999999999999E-3,2.9340000000000002,351.6,2487,351.7,2298,2650]
[86,0.60109999999999997,1.0330000000000001E-3,2.7269999999999999,360,2489,360.1,2293,2653]
[88,0.64949999999999997,1.034E-3,2.536,368.4,2491,368.5,2288,2656]
[90,0.70109999999999995,1.036E-3,2.3610000000000002,376.9,2493,377,2282,2659]
[92,0.75600000000000001,1.0369999999999999E-3,2.2000000000000002,385.3,2496,385.4,2277,2662]
[94,0.8145,1.039E-3,2.052,393.7,2499,393.8,2272,2666]
[96,0.87670000000000003,1.0399999999999999E-3,1.915,402.1,2501,402.2,2267,2669]
[98,0.94289999999999996,1.042E-3,1.7889999999999999,410.6,2504,410.7,2262,2673]
[100,1.0130999999999999,1.044E-3,1.673,419,2507,419.1,2257,2676]
[102,1.0875999999999999,1.0449999999999999E-3,1.5660000000000001,427.1,2509,427.5,2251,2679]

{"sheet":"B7","index":21,"n_rows":57,"n_cols":20,"rows_kept":57,"cut":false,"hidden":true,"merged":[]}
["P(Tsat)","SatW","SatS",50,75,100,150,200,250,300,350,400,450,500,550,600,650,700,750,"H"]
[0,"—","—",2595,2642,2689,2784,2880,2978,3077,3177,3280,3384,3497,3597,3706,3816,3929,4043]
[0.1,191.8,2584.8000000000002,2593,2640,2688,2783,2880,2977,3077,3177,3280,3384,3489,3596,3706,3816,3929,4043]
[0.5,340.6,2646,null,null,2683,2780,2878,2979,3076,3177,3279,3383,3489,3596,3705,3816,3929,4043]
[1,417.5,2675.4,null,null,2676,2776,2875,2975,3074,3176,3278,3382,3488,3596,3705,3816,3928,4042]
[5,640.1,2747.5,null,null,null,null,2855,2961,3065,3168,3272,3379,3484,3592,3702,3813,3926,4040]
[10,762.6,2776.2,null,null,null,null,2827,2943,3052,3159,3264,3371,3478,3587,3697,3809,3923,4038]
[20,908.6,2797.2,null,null,null,null,null,2902,3025,3139,3249,3358,3467,3578,3689,3802,3916,4032]
[40,1087.4000000000001,2800.3,null,null,null,null,null,null,2962,3095,3216,3331,3445,3559,3673,3788,3904,4021]
[60,1213.7,2785,null,null,null,null,null,null,2885,3046,3180,3303,3422,3539,3657,3774,3892,4011]
[80,1317.1,2759.9,null,null,null,null,null,null,2787,2990,3142,3274,3399,3520,3640,3759,3879,4000]
[100,1408,2727.7,null,null,null,null,null,null,null,2926,3100,3244,3375,3500,3623,3745,3867,3989]
[150,1611,2615,null,null,null,null,null,null,null,2695,2975,3160,3311,3448,3580,3708,3835,3962]
[200,1826.5,2418.4,null,null,null,null,null,null,null,null,2820,3064,3241,3394,3536,3671,3804,3935]
[221.2,2108,2108,null,null,null,null,null,null,null,null,2733,3020,3210,3370,3516,3655,3790,3923]
[250,"—","—",230.7,334,437.8,647.70000000000005,862.8,1087.5,1331.1,1625,2582,2954,3166,3337,3490,3633,3772,3908]
[300,"—","—",235,338.1,441.6,650.9,865.2,1088.4000000000001,1328.7,1609.9,2162,2826,3085,3277,3443,3595,3740,3880]
[500,"—","—",251.9,354.2,456.8,664.1,875.4,1093.5999999999999,1323.7,1576.3,1878,2293,2723,3021,3248,3439,3610,3771]
[1000,"—","—",293.89999999999998,394.3,495.1,698,903.5,1113,1328.7,1550.5,1798,2051,2316,2594,2857,3105,3324,3526]
["P(Tsat)","SatW","SatS",50,75,100,150,200,250,300,350,400,450,500,550,600,650,700,750,"U"]
[0,"—","—",2446,2481,2517,2589,2662,2736,2812,2890,2969,3050,3132,3217,3303,3390,3480,3591]
[0.1,191.8,2438,2444,2480,2516,2588,2661,2736,2812,2890,2969,3050,3132,3217,3303,3390,3480,3571]
[0.5,340.6,2484,null,null,2512,2586,2660,2735,2811,2889,2969,3049,3132,3216,3302,3390,3480,3571]
[1,417.5,2506.1,null,null,2507,2583,2658,2734,2811,2889,2968,3049,3132,3216,3302,3390,3479,3570]
[5,639.6,2560.1999999999998,null,null,null,null,2643,2724,2803,2883,2964,3045,3128,3213,3300,3388,3477,3569]
[10,761.5,2582,null,null,null,null,2621,2710,2794,2876,2958,3041,3124,3210,3296,3385,3475,3567]
[20,906.2,2598.1999999999998,null,null,null,null,null,2679,2774,2862,2946,3031,3115,3202,3290,3379,3470,3562]
[40,1082.4000000000001,2601.3000000000002,null,null,null,null,null,null,2727,2829,2922,3011,3100,3188,3278,3368,3460,3554]
[60,1205.8,2590.4,null,null,null,null,null,null,2668,2792,2896,2991,3083,3174,3265,3357,3451,3545]
[80,1306,2571.6999999999998,null,null,null,null,null,null,2593,2750,2867,2969,3065,3159,3252,3346,3441,3537]
[100,1393.5,2547.3000000000002,null,null,null,null,null,null,null,2702,2836,2946,3047,3144,3240,3335,3431,3528]
[150,1586.1,2459.9,null,null,null,null,null,null,null,2523,2744,2883,2999,3105,3207,3307,3407,3507]
[200,1785.7,2300.8000000000002,null,null,null,null,null,null,null,null,2622,2810,2946,3063,3172,3278,3382,3485]
[221.2,2037.8,2037.8,null,null,null,null,null,null,null,null,2553,2776,2922,3045,3157,3265,3371,3476]
[250,"—","—",205.7,308.7,412.1,620.79999999999995,834.4,1057,1297.5,1585,2432,2725,2888,3019,3137,3248,3356,3463]
[300,"—","—",205,307.7,410.8,618.70000000000005,831.3,1052.0999999999999,1288.7,1563.3,2077,2623,2825,2972,3100,3218,3330,3441]
[500,"—","—",202.4,304,405.8,611,819.7,1034.3,1259.3,1504.1,1791,2169,2529,2765,2946,3091,3224,3350]
[1000,"—","—",196.5,295.7,395.1,594.4,795.3,999,1207.0999999999999,1419,1653,1888,2127,2369,2591,2795,2971,3131]
["P(Tsat)","SatW","SatS",50,75,100,150,200,250,300,350,400,450,500,550,600,650,700,750,"V"]
[0]
[0.1,1.01E-3,14.7,14.8,16,17.2,19.5,21.8,24.2,26.5,28.7,21.1,33.299999999999997,35.700000000000003,38,40.299999999999997,42.6,44.8,47.2]
[0.5,1.0300000000000001E-3,3.24,null,null,3.41,3.89,4.3499999999999996,4.83,5.29,5.75,6.21,6.67,7.14,7.58,8.06,8.5500000000000007,9.01,9.43]
[1,1.0399999999999999E-3,1.69,null,null,1.69,1.94,2.17,2.4,2.64,2.87,3.11,3.33,3.57,3.8,4.03,4.26,4.4800000000000004,4.72]
[5,1.09E-3,0.375,null,null,null,null,0.42499999999999999,0.47399999999999998,0.52200000000000002,0.57099999999999995,0.61699999999999999,0.66400000000000003,0.71099999999999997,0.75800000000000001,0.80400000000000005,0.85,0.89700000000000002,0.94299999999999995]
[10,1.1299999999999999E-3,0.19400000000000001,null,null,null,null,0.20599999999999999,0.23300000000000001,0.25800000000000001,0.28199999999999997,0.307,0.33,0.35299999999999998,0.377,0.40200000000000002,0.42399999999999999,0.44800000000000001,0.47199999999999998]
[20,1.1800000000000001E-3,9.9500000000000005E-2,null,null,null,null,null,0.111,0.125,0.13900000000000001,0.151,0.16300000000000001,0.17499999999999999,0.188,0.2,0.21099999999999999,0.223,0.23499999999999999]
[40,1.25E-3,4.9750000000000003E-2,null,null,null,null,null,null,5.8799999999999998E-2,6.6500000000000004E-2,7.3400000000000007E-2,7.9899999999999999E-2,8.6400000000000005E-2,9.2600000000000002E-2,9.8699999999999996E-2,0.105,0.111,0.11700000000000001]
[60,1.32E-3,3.2500000000000001E-2,null,null,null,null,null,null,3.61E-2,4.2200000000000001E-2,4.7399999999999998E-2,5.21E-2,5.6599999999999998E-2,6.0900000000000003E-2,6.5199999999999994E-2,6.93E-2,7.3499999999999996E-2,7.7600000000000002E-2]
[80,1.39E-3,2.35E-2,null,null,null,null,null,null,2.4299999999999999E-2,2.9899999999999999E-2,3.44E-2,3.8199999999999998E-2,4.1700000000000001E-2,4.4999999999999998E-2,4.8300000000000003E-2,5.1499999999999997E-2,5.4699999999999999E-2,5.7799999999999997E-2]
[100,1.4499999999999999E-3,1.8100000000000002E-2,null,null,null,null,null,null,null,2.24E-2,2.64E-2,2.98E-2,3.2800000000000003E-2,3.56E-2,3.8300000000000001E-2,4.1000000000000002E-2,4.3499999999999997E-2,4.6100000000000002E-2]
[150,1.66E-3,1.03E-2,null,null,null,null,null,null,null,1.15E-2,1.5699999999999999E-2,1.8499999999999999E-2,2.0799999999999999E-2,2.29E-2,2.4899999999999999E-2,2.6700000000000002E-2,2.86E-2,3.04E-2]
[200,2.0400000000000001E-3,5.875E-3,null,null,null,null,null,null,null,null,9.9500000000000005E-3,1.2699999999999999E-2,1.4800000000000001E-2,1.66E-2,1.8200000000000001E-2,0.19700000000000001,0.21099999999999999,2.2499999999999999E-2]
[221.2,3.1700000000000001E-3,3.1700000000000001E-3,null,null,null,null,null,null,null,null,8.1569999999999993E-3,1.0999999999999999E-2,1.2999999999999999E-2,1.47E-2,1.6199999999999999E-2,1.7600000000000001E-2,1.9E-2,2.0199999999999999E-2]
[250,"—","—",1E-3,1.01E-3,1.0300000000000001E-3,1.08E-3,1.1299999999999999E-3,1.2199999999999999E-3,1.3500000000000001E-3,1.6000000000000001E-3,6.0130000000000001E-3,9.1739999999999999E-3,1.11E-2,1.2699999999999999E-2,1.41E-2,1.43E-2,1.66E-2,1.78E-2]
[300,"—","—",9.990000000000001E-4,1.01E-3,1.0300000000000001E-3,1.07E-3,1.1299999999999999E-3,1.2099999999999999E-3,1.33E-3,1.5499999999999999E-3,2.8300000000000001E-3,6.7340000000000004E-3,8.6800000000000002E-3,1.0200000000000001E-2,1.14E-2,1.26E-2,1.3599999999999999E-2,1.47E-2]
[500,"—","—",9.9109999999999997E-4,1E-3,1.0200000000000001E-3,1.06E-3,1.1100000000000001E-3,1.1900000000000001E-3,1.2899999999999999E-3,1.4400000000000001E-3,1.7260000000000001E-3,2.4910000000000002E-3,3.882E-3,5.1120000000000002E-3,6.1120000000000002E-3,7.0000000000000001E-3,7.7219999999999997E-3,8.4180000000000001E-3]
[1000,"—","—",9.7369999999999998E-4,9.8520000000000009E-4,1E-3,1.0399999999999999E-3,1.08E-3,1.14E-3,1.2199999999999999E-3,1.31E-3,1.446E-3,1.6280000000000001E-3,1.8929999999999999E-3,2.2460000000000002E-3,2.6679999999999998E-3,3.1059999999999998E-3,3.5360000000000001E-3,3.9529999999999999E-3]

{"sheet":"B7L","index":22,"n_rows":57,"n_cols":20,"rows_kept":57,"cut":false,"hidden":true,"merged":[]}
["P(Tsat)","SatW","SatS",50,75,100,150,200,250,300,350,400,450,500,550,600,650,700,750,"H"]
[0,"—","—"]
[0.1,191.8,2584.8000000000002]
[0.5,340.6,2646,209.3,313.89999999999998]
[1,417.5,2675.4,209.3,314]
[5,640.1,2747.5,209.7,314.3,419.4,632.20000000000005]
[10,762.6,2776.2,210.1,314.7,419.7,632.5]
[20,908.6,2797.2,211,315.5,420.5,633.1,852.6]
[40,1087.4000000000001,2800.3,212.7,317.10000000000002,422,634.29999999999995,853.4,1085.8]
[60,1213.7,2785,214.4,318.7,423.5,635.6,854.2,1085.8]
[80,1317.1,2759.9,216.1,320.3,425,636.79999999999995,855.1,1085.8]
[100,1408,2727.7,217.8,322.89999999999998,426.5,638.1,855.9,1085.8,1343.4]
[150,1611,2615,222.1,326,430.3,641.29999999999995,858.1,1086.2,1338.2]
[200,1826.5,2418.4,226.4,330,434,644.5,860.4,1086.7,1334.3,1647.1]
[221.2,2108,2108,228.2,331.7,435.7,645.79999999999995,861.4,1087,1332.8,1635.5]
[250,"—","—"]
[300,"—","—"]
[500,"—","—"]
[1000,"—","—"]
["P(Tsat)","SatW","SatS",50,75,100,150,200,250,300,350,400,450,500,550,600,650,700,750,"U"]
[0,"—","—"]
[0.1,191.8,2438]
[0.5,340.6,2484,209.2,313.89999999999998]
[1,417.5,2506.1,209.2,313.89999999999998]
[5,639.6,2560.1999999999998,209.2,313.8,418.8,631.6]
[10,761.5,2582,209.1,313.7,418.7,631.4]
[20,906.2,2598.1999999999998,209,313.5,418.4,603.9,850.2]
[40,1082.4000000000001,2601.3000000000002,208.6,313,417.8,630,848.8,1080.8]
[60,1205.8,2590.4,208.3,312.60000000000002,417.3,629.1,847.3,1078.3]
[80,1306,2571.6999999999998,208.1,312.3,416.7,628.20000000000005,845.9,1075.8]
[100,1393.5,2547.3000000000002,207.8,311.7,416.1,627.29999999999995,844.4,1073.4000000000001,1329.4]
[150,1586.1,2459.9,207,310.7,414.7,625,841,1067.7,1317.6]
[200,1785.7,2300.8000000000002,206.3,309.7,413.2,622.9,837.7,1062.2,1307.0999999999999,1613.7]
[221.2,2037.8,2037.8,206,309.2,412.8,622,836.3,1060,1302.9000000000001,1600.3]
[250,"—","—"]
[300,"—","—"]
[500,"—","—"]
[1000,"—","—"]
["P(Tsat)","SatW","SatS",50,75,100,150,200,250,300,350,400,450,500,550,600,650,700,750,"V"]
[0]
[0.1,1.01E-3,14.7]
[0.5,1.0300000000000001E-3,3.24,1.01E-3,1.0300000000000001E-3]
[1,1.0399999999999999E-3,1.69,1.01E-3,1.0300000000000001E-3]
[5,1.09E-3,0.375,1.01E-3,1.0300000000000001E-3,1.0399999999999999E-3,1.09E-3]
[10,1.1299999999999999E-3,0.19400000000000001,1.01E-3,1.0300000000000001E-3,1.0399999999999999E-3,1.09E-3]
[20,1.1800000000000001E-3,9.9500000000000005E-2,1.01E-3,1.0200000000000001E-3,1.0399999999999999E-3,1.09E-3,1.16E-3]
[40,1.25E-3,4.9750000000000003E-2,1.01E-3,1.0200000000000001E-3,1.0399999999999999E-3,1.09E-3,1.15E-3,1.25E-3]
[60,1.32E-3,3.2500000000000001E-2,1.01E-3,1.0300000000000001E-3,1.0399999999999999E-3,1.09E-3,1.15E-3,1.25E-3]
[80,1.39E-3,2.35E-2,1.01E-3,1.0200000000000001E-3,1.0399999999999999E-3,1.09E-3,1.15E-3,1.24E-3]
[100,1.4499999999999999E-3,1.8100000000000002E-2,1.01E-3,1.0200000000000001E-3,1.0399999999999999E-3,1.09E-3,1.15E-3,1.24E-3,1.4E-3]
[150,1.66E-3,1.03E-2,1.01E-3,1.0200000000000001E-3,1.0399999999999999E-3,1.08E-3,1.14E-3,1.23E-3,1.3799999999999999E-3]
[200,2.0400000000000001E-3,5.875E-3,1E-3,1.0200000000000001E-3,1.0300000000000001E-3,1.08E-3,1.14E-3,1.2199999999999999E-3,1.3600000000000001E-3,1.67E-3]
[221.2,3.1700000000000001E-3,3.1700000000000001E-3,1E-3,1.0200000000000001E-3,1.0300000000000001E-3,1.08E-3,1.14E-3,1.2199999999999999E-3,1.3500000000000001E-3,1.6299999999999999E-3]
[250,"—","—"]
[300,"—","—"]
[500,"—","—"]
[1000,"—","—"]

{"sheet":"Steam Tables","index":23,"n_rows":28,"n_cols":13,"rows_kept":28,"cut":false,"hidden":true,"merged":[]}
["ST"]
[]
["Temperature","P",null,102]
[{"$f":"[0]!SteamSatT(50,\"t\",\"p\")","v":{"$error":"#VALUE!"}},null,null,"T"]
[{"$f":"[0]!SteamSatT(51,\"t\",\"p\")","v":{"$error":"#VALUE!"}},{"$f":"+(0.1361+0.1234)/2","v":0.12975},null,"h",null,null,null,null,null,"Input ",40,"P"]
[null,null,null,"e",null,null,null,null,null,"Input2",1.06E-3,"V"]
[null,null,null,{"$f":"[0]!SteamSatT(D3,D4,D5,D6)","v":{"$error":"#VALUE!"}},null,null,{"$f":"[0]!SteamSH(90,625,\"P\",\"T\",\"H\")","v":{"$error":"#VALUE!"}},{"$f":"3640+3759","v":7399},{"$f":"[0]!SteamSH(625,90,\"T\",\"P\",\"H\")","v":{"$error":"#VALUE!"}},"T",{"$f":"[0]!SteamSH(K5,K6,L5,L6,J7,\"l\")","v":{"$error":"#VALUE!"}},null,{"$f":"MATCH(3252, 'B7'!P21:P38, -1)","v":10}]
[null,null,null,null,null,null,{"$f":"[0]!SteamSH(90,600,\"P\",\"T\",\"H\")","v":{"$error":"#VALUE!"}},{"$f":"+H7/2","v":3699.5},{"$f":"[0]!SteamSH(90,600,\"P\",\"T\",\"H\")","v":{"$error":"#VALUE!"}}]
["Pressure",null,null,102,null,null,{"$f":"[0]!SteamSH(90,650,\"P\",\"T\",\"H\")","v":{"$error":"#VALUE!"}},null,{"$f":"[0]!SteamSH(90,650,\"P\",\"T\",\"H\")","v":{"$error":"#VALUE!"}}]
[{"$f":"[0]!SteamSatP(1.1,\"p\",\"t\")","v":{"$error":"#VALUE!"}},null,null,"T",null,null,{"$f":"AVERAGE(G8:G9)","v":{"$error":"#VALUE!"}}]
[{"$f":"[0]!SteamSatP(51,\"t\",\"p\")","v":{"$error":"#VALUE!"}},{"$f":"+(0.1361+0.1234)/2","v":0.12975},null,"h",null,null,null,null,null,null,null,3303,{"$f":"MATCH(3240,L11:L28,-1)","v":11}]
[null,null,null,"e",null,null,null,null,null,null,null,3303]
[null,null,null,{"$f":"[0]!SteamSatP(D9,D10,D11,D12)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,3302]
[null,null,null,null,null,null,null,null,null,null,null,3302]
[null,null,null,null,null,null,null,null,null,null,null,3300]
[null,null,null,null,null,{"$f":"[0]!SteamSatP(20,\"P\",\"U\",\"V\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,3296]
[null,null,null,null,null,{"$f":"[0]!SteamSatP(2598.2,\"U\",\"P\",\"V\",\"U\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,3290]
[null,null,null,null,null,{"$f":"[0]!SteamSatP(2598.2,\"U\",\"H\",\"V\",\"U\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,3278]
[null,null,null,null,null,{"$f":"[0]!SteamSatP(2787,\"H\",\"P\",\"V\",\"U\")","v":{"$error":"#VALUE!"}},null,null,null,null,null,3265]
[null,{"$f":"[0]!Enthalpy(\"Benzene\",10,80.1)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,3252]
[null,{"$f":"[0]!AntoineP(\"ethanol\", 10)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,3240]
[null,{"$f":"[0]!AntoineT(\"ethanol\",B21)","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,3207]
[null,null,null,null,null,null,null,null,null,null,null,3172]
[null,null,null,null,null,null,null,null,null,null,null,3157]
[null,null,null,null,null,null,null,null,null,null,null,3137]
[null,null,null,null,null,null,null,null,null,null,null,3100]
[null,null,null,null,null,null,null,null,null,null,null,2946]
[null,null,null,null,null,null,null,null,null,null,null,2591]

{"sheet":"Species","index":24,"n_rows":177,"n_cols":12,"rows_kept":177,"cut":false,"hidden":false,"merged":[]}
["Text Name","CAS","Formula","Synonyms, tradenames, variations",null,null,null,"Source: en.wikipedia.org, CDC-NIOSH Pocket Guide to Chemical Hazards"]
["acetaldehyde","75-07-0","CH3CHO","Acetic aldehyde","Ethanal","Ethyl aldehyde","C2H4O"]
["acetic acid","64-19-7","CH3COOH","Acetic acid (aqueous)","Ethanoic acid","Glacial acetic acid","Methanecarboxylic acid","vinegar","C2H4O2"]
["acetic anhydride","108-24-7","(CH3CO)2O","Acetic acid anhydride","Acetic oxide","Acetyl oxide","Ethanoic anhydride","C4H6O3"]
["acetone","67-64-1","(ch3)2co","dimethyl ketone","2-propanone","ketone propane","","","","",""]
["acetylene","74-86-2","c2h2","ethine","ethyne","hcch","hc≡ch ","","","",""]
["acrylic acid","79-10-7","CH2CHCOOH","CH2=CHCOOH","Acroleic acid","Aqueous acrylic acid","Ethylenecarboxylic acid","Glacial acrylic acid","2-Propenoic acid","C3H4O2",""]
["air","","","","","","","","","",""]
["ammonia","7664-41-7","nh3","anhydrous ammonia","aqua ammonia","aqueous ammonia","","","","",""]
["ammonium hydroxide","1336-21-6","NH4OH","ammonia water","ammonical liquor","ammonia liquor","aqua ammonia","","","",""]
["ammonium nitrate","6484-52-2","(NH4)(NO3)","NH4NO3","","","","","","",""]
["ammonium sulfate","7783-20-2","(nh4)2so4","ammonium sulphate","diazanium sulfate","diammonium sulfate","sulfuric acid diammonium salt","mascagnite","actamaster","dolamin",""]
["aniline","62-53-3","C6H5NH2","Aminobenzene","Aniline oil","Benzenamine","Phenylamine","C6H7N","","",""]
["benzaldehyde","100-52-7","C7H6O","Phenylmethanal","Benzenecarboxaldehyde","Benzoic aldehyde","","","","",""]
["benzene","71-43-2","c6h6","phenyl hydride","benzol","","","","","",""]
["benzoic acid","65-85-0","C6H5COOH","Carboxybenzene","Benzenecarboxylic acid","Dracylic acid","","","","",""]
["benzyl alcohol","100-51-6","C7H8O","Phenylmethanol","Phenylcarbinol","","","","","",""]
["1,2-butadiene","590-19-2","C4H6","Methylallene","","","","","","",""]
["1,3-butadiene","106-99-0","CH2CHCHCH2","CH2=CHCH=CH2","Biethylene","Bivinyl","Butadiene","Divinyl","Erythrene","Vinylethylene","C4H6"]
["bromine","7726-95-6","Br2","Molecular bromine","","","","","","",""]
["isobutane","75-28-5","c4h10","2-methylpropane","i-butane","differs on b1, b4","","","","",""]
["n-butane","106-97-8","c4h10","normal-butane","butyl hydride","ch3ch2ch2ch3","diethyl","methylethylmethane","","",""]
["1-butanol","71-36-3","C4h9OH","n-Butyl alcohol","CH3CH2CH2CH2OH","C4H10O","n-Butanol","Butyl alcohol","1-Hydroxybutane","n-Propyl carbinol",""]
["2-butanol","78-92-2","CH3CH(OH)CH2CH3","sec-Butyl alcohol","Butylene hydrate","2-Hydroxybutane","Methyl ethyl carbinol","C4H10O","C4H9OH","",""]
["1-butene","106-98-9","C4H8","but-1-ene","ethylethylene","1-butylene","α-butylene","but-1-ene","","",""]
["butyric acid","107-92-6","C4H8O2","Butanoic acid","1-Propanecarboxylic acid","Propanecarboxylic acid","",null,"","",""]
["isobutene","115-11-7","c4h8","2-methylpropene","γ-butylene","2-methylpropylene","isobutylene","","","",""]
["calcium carbide","75-20-7","cac2","calcium acetylide","calcium dicarbide","","","","","",""]
["calcium carbonate","471-34-1","caco3","1317-65-3","","","","","","",""]
["calcium chloride","10043-52-4","CaCl2","Calcium dichloride","Calcium(II) chloride","","","","","",""]
["calcium hydroxide","1305-62-0","ca(oh)2","calcium hydrate","caustic lime","hydrated lime","slaked lime","","","",""]
["calcium oxide","1305-78-8","cao","burned lime","burnt lime","lime","pebble lime","quick lime","unslaked lime","",""]
["calcium phosphate","7758-87-4","Ca3(PO4)2","tricalcium diphosphate","Ca3O8P2","","","","","",""]
["calcium silicate","1344-95-2","CaSiO3","Calcium hydrosilicate","Calcium metasilicate","Calcium monosilicate","","","","",""]
["calcium suflate","7778-18-9","CaSO4","gypsum","Anhydrous calcium sulfate","Anhydrous gypsum","","","","",""]
["carbon","1333-86-4","c","1333-86-4","carbon black","acetylene black","channel black","furnace black","lamp black","thermal black","graphite","carbon (graphite)"]
["carbon dioxide","124-38-9","co2","carbonic acid gas","dry ice","","","","","",""]
["carbon disulfide","75-15-0","CS2","Carbon bisulfide","","","","","","",""]
["carbon monoxide","630-08-0","co","flue gas","monoxide","","","","","",""]
["carbon tetrachloride","56-23-5","ccl4","carbon chloride","carbon tet","freon® 10","halon® 104","tetrachloromethane","freon 10","freon10","halon10"]
["chlorine","7782-50-5","cl2","molecular chlorine","","","","","","",""]
["chlorbenzene","108-90-7","C6H5Cl","Benzene chloride","Chlorobenzol","MCB","Monochlorobenzene","Phenyl chloride","","",""]
["chloroform","67-66-3","CHCl3","Methane trichloride","Trichloromethane","","","","","",""]
["copper","7440-50-8","cu","copper metal dusts","copper metal fumes","","","","","",""]
["cupric sulfate","7758-98-7","CuSO4","Copper(II) sulfate","Cupper(II)sulphate","Blue vitriol","Bluestone","Chalcanthite","","",""]
["cumene","98-82-8","c6h5ch(ch3)2","isopropyl benzene","cumol","2-phenyl propane","","","","",""]
["cyclohexane","110-82-7","c6h12","benzene hexahydride","hexahydrobenzene","hexamethylene","hexanaphthene","","","",""]
["cyclohexanol","108-93-0","C6H11OH","Anol","Cyclohexyl alcohol","","","","","",""]
["cyclopentane","287-92-3","c5h10","pentamethylene","Hexahydrophenol","Hexalin","Hydralin","Hydroxycyclohexane","","",""]
["n-decane","124-18-5","C10H22","decane","","","","","","",""]
["1-decene","872-05-9","C10H20","decene","","","","","","",""]
["diethyl ether","60-29-7","C2H5OC2H5","Ethyl ether","Diethyl oxide","Ethyl oxide","Ether","Solvent ether","","",""]
["1,1-dichloroethane","75-34-3","CHCl2CH3","Asymmetrical dichloroethane","Ethylidene chloride","1,1-Ethylidene dichloride","","","","",""]
["1,2-dichloroethane","107-06-2","ClCH2CH2Cl","Ethylene dichloride","Ethylene chloride","Glycol dichloride","","","","",""]
["dichloromethane","75-09-2","CH2Cl2","Methylene chloride","Methylene dichloride","","","","","",""]
["diethyl ketone","96-22-0","CH3CH2COCH2CH3","DEK","Dimethylacetone","Ethyl ketone","Metacetone","3-Pentanone","Propione","",""]
["diethylene glycol","111-46-6","C4H10O3","(2-hydroxyethoxy)ethan-2-ol","ethylene diglycol","diglycol","dihydroxy diethyl ether","","","",""]
["dimethyl ether","115-10-6","C2H6O","DME","Wood ether","Methyl ether","Dymel A","Dimethyl oxide","Demeon","Methoxymethane",""]
["dimethylamine","124-40-3","(CH3)2NH","N-Methylmethanamine","","","","","","",""]
["n,n-dimethylformamide","68-12-2 ","C3H7NO","N,N-dimethylmethanamide","DMF","dimethylformamide","DMFA","","","",""]
["1,4-dioxane","123-91-1","C4H8O2","Diethylene dioxide","Diethylene ether","Dioxan","p-Dioxane","Dioxane","","",""]
["ethane","74-84-0","c2h6","","","","","","","",""]
["ethyl acetate","141-78-6","CH3COOC2H5","Acetic ester","Acetic ether","Ethyl ethanoate","","","","",""]
["ethyl alcohol","64-17-5","ch3ch2oh","ethanol","alcohol","cologne spirit","etoh","grain alcohol","c2h6o","c2h5oh","deffers in b1,b4"]
["ethyl benzene","100-41-4","CH3CH2C6H5","Ethylbenzol","Phenylethane","ethylbenzene","","","","","differs in b1, b4"]
["ethyl bromide","74-96-4","CH3CH2Br","Bromoethane","Monobromoethane","","","","","",""]
["ethyl chloride","75-00-3","CH3CH2Cl","chloroethane","Hydrochloric ether","Monochloroethane","Muriatic ether","","","",""]
["3-ethyl hexane","619-99-8","C8H18","3-ethylhexane","","","","","","",""]
["ethanolamine","141-43-5","NH2CH2CH2OH","2-Aminoethanol","β-Aminoethyl alcohol","Ethylolamine","2-Hydroxyethylamine","Monoethanolamine","","",""]
["ethylene","74-85-1","c2h4","ethene","","","","","","",""]
["ethylene glycol","107-21-1","HOCH2CH2OH","1,2-Dihydroxyethane","1,2-Ethanediol","Glycol","Glycol alcohol","Monoethylene glycol","","",""]
["ethylene oxide","75-21-8","C2H4O","Dimethylene oxide","1,2-Epoxy ethane","Oxirane","","","","",""]
["1,2-ethylenediamine","107-15-3","NH2CH2CH2NH2","Ethylenediamine","1,2-Diaminoethane","1,2-Ethanediamine","","","","",""]
["ferric oxide","1309-37-1","fe2o3","iron(iii) oxide","","","","","","",""]
["ferrous oxide","1345-25-1","FeO","Iron(II) oxide","","","","","","",""]
["ferrous sulfide","1317-37-9","FeS","Iron(II) sulfide","Iron sulfide","black iron sulfide","","","","",""]
["formaldehyde","50-00-0","hcho","h2co","methanal","methyl aldehyde","methylene oxide","","","",""]
["formic acid","64-18-6","CH2O2","Methanoic acid","Aminic acid","Formylic acid","Hydrogen carboxylic acid","Hydroxymethanone","Hydroxy(oxo)methane","Metacarbonoic acid","Oxomethanol","Oxocarbinic acid"]
["glycerol","56-81-5","HOCH2CH(OH)CH2OH","Glycerin","Glycyl alcohol","1,2,3-Propanetriol","Trihydroxypropane","","","",""]
["helium","7440-59-7","he","","","","","","","",""]
["n-heptane","142-82-5","CH3((CH2)5CH3","heptane","normal-heptane","","","","","",""]
["i-heptane","591-76-4","C7H16","2-Methylhexane","isoheptane","ethylisobutylmethane","","","","",""]
["1-heptene","592-76-7","C7H14","heptene","hept-1-ene","","","","","",""]
["n-hexane","110-54-3","c614","ch3(ch2)4ch3","hexane","hexyl hydride","normal-hexane","normal hexane","","",""]
["i-hexane","107-83-5","C6H14","2-methylpentane","isohexane","","","","","",""]
["1-hexene","592-41-6","C6H12","Hex-1-ene","Hexene","Hexylene","butyl ethylene","","","",""]
["hydrogen","1333-74-0","h2","","","","","","","",""]
["hydrogen bromide","10035-10-6","hbr","anhydrous hydrogen bromide","aqueous hydrogen bromide","hydrobromic acid","","","","",""]
["hydrogen chloride","7647-01-0","hcl","anhydrous hydrogen chloride","aqueous hydrogen chloride","hydrochloric acid","muriatic acid","","","",""]
["hydrogen cyanide","74-90-8","hcn","formonitrile","hydrocyanic acid","prussic acid","","","","",""]
["hydrogen fluoride","7664-39-3","HF","HF-A","hydrofluoric acid","","","","","",""]
["hydrogen sulfide","7783-06-4","h2s","hydrosulfuric acid","sewer gas","sulfuretted hydrogen","","","","",""]
["iodine","7553-56-2","I2","7553-56-2","","","","","","",""]
["iron","7439-89-6","Fe","ferrum","","","","","","",""]
["lead","7439-92-1","Pb","Plumbum","","","","","","",""]
["lead oxide","1317-36-8","PbO","Lead(II) oxide","Lead monoxide","Lead monoxide","Massicot","Plumbous oxide","","",""]
["magnesium","7439-95-4","Mg","","","","","","","",""]
["magnesium chloride","7786-30-3","mgcl2","magnesium dichloride","","","","","","",""]
["magnesium hydroxide","1309-42-8","Mg(OH)2","Milk of Magnesia","","","","","","",""]
["magnesium oxide","1309-48-4","mgo","","","","","","","",""]
["mercury","7439-97-6","hg","","","","","","","",""]
["methane","74-82-8","ch4","methyl hydride","marsh gas","biogas","","","","",""]
["methyl acetate","79-20-9","CH3COOCH3","Methyl ethanoate","","","","","","",""]
["methyl alcohol","67-56-1","ch3oh","carbinol","columbian spirits","methanol","pyroligneous spirit","wood alcohol","wood naphtha","wood spirit","differs in b1, b4"]
["methyl amine","74-89-5","CH3NH2","Methylamine","Aminomethane","Monomethylamine","","","","","differs in b1, b4"]
["methyl bromide","74-83-9","CH3Br","Bromomethane","Monobromomethane","Halon 1001","Curafume","Embafume","Terabol","",""]
["methyl chloride","74-87-3","CH3Cl","Chloromethane","Monochloromethane","","","","","",""]
["methyl cyclohexane","108-87-2","ch3c6h11","methylcyclohexane","c7h14","","","","","","differs in b1, b4"]
["methyl cyclopentane","96-37-7","ch3c5h9","methylcyclopentane","c6h12","","","","","",""]
["methyl ethyl ketone","78-93-3","CH3COCH2CH3","Ethyl methyl ketone","MEK","2-Butanone","Methyl acetone","","","",""]
["methyl isobutyl ketone","108-10-1","CH3COCH2CH(CH3)2","Isobutyl methyl ketone","Hexone","4-Methyl 2-pentanone","MIBK","","","",""]
["methyl methacrylate","80-62-6","CH2C(CH3)COOCH3","Methacrylate monomer","Methyl-2-methyl-2-propenoate","","","","","",""]
["napthalene","91-20-3","C10H8","Naphthalin","Tar camphor","White tar ","","","","",""]
["nickel","7440-02-0","Ni","","","","","","","",""]
["nitric acid","7697-37-2","hno3","aqua fortis","engravers acid","hydrogen nitrate","","","","",""]
["nitric oxide","10102-43-9","no","mononitrogen monoxide","nitrogen monoxide","","","","","",""]
["nitromethane","75-52-5","CH3NO2","Nitrocarbol","","","","","","",""]
["nitrobenzene","98-95-3","C6H5NO2","Essence of mirbane","Oil of mirbane","Nitrobenzol","","","","",""]
["nitrogen","7727-37-9","n2","","","","","","","",""]
["nitrogen dioxide","10102-44-0","no2","nitrogen peroxide","","","","","","",""]
["nitrogen pentoxide","10102-03-1","N2O5","Nitric acid anhydride","Dinitrogen pentaoxide","","","","","",""]
["nitrogen tetraoxide","10544-72-6","n2o4","dinitrogen tetroxide","nitrogen tetroxide","nitrogen peroxide","","","","",""]
["nitrous oxide","10024-97-2","n2o","dinitrogen monoxide","hyponitrous acid anhydride","laughing gas","","","","",""]
["n-nonane","111-84-2","CH3(CH2)7CH3","Nonyl hydride","Nonane","","","","","",""]
["1-nonene","124-11-8","C9H18","alpha-Nonene","nonene","Non-1-ene","","","","",""]
["n-octane","111-65-9","CH3(CH2)6CH3","normal-Octane","normal Octane","octane","","","","",""]
["i-octane","540-84-1","C8H18","2,2,4-Trimethylpentane","isooctane","I octane","","","","",""]
["1-octene","111-66-0","C8H16","Oct-1-ene","octene","octylene","Octene-1","1-n-ctene","hexylethylene","",""]
["oxalic acid","144-62-7","HOOCCOOH • 2H2O","Ethanedioic acid","Oxalic acid dihydrate","","","","","",""]
["oxygen","7782-44-7","o2","","","","","","","",""]
["n-pentane","109-66-0","c5h12","pentane","normal-pentane","ch3(ch2)3ch3","","","","",""]
["isopentane","78-78-4","C5H12","i-pentane","2-Methylbutane","Methylbutane","","","","","differs in b1, b4"]
["1-pentanol","71-41-0","C5H12O","C5H11OH","Amyl alcohol","pentanol","Amylic alcohol","Butylcarbinol","Hydroxypentane","n-pentanol","Pentalcohol"]
["1-pentene","109-67-1","C5H10","Propylethylene","","","","","","",""]
["phenol","108-95-2","C6H5OH","Carbolic acid","Hydroxybenzene","Monohydroxybenzene","Phenyl alcohol","Phenyl hydroxide","","",""]
["phosphoric acid","7664-38-2","H3PO4","Orthophosphoric acid","White phosphoric acid","","","","","",""]
["phosphorus (red)","7723-14-0","P","red phosphorus","phosphorus","","","","","",""]
["phosphorus (white)","7723-14-0","P","white phosphorus","","","","","","",""]
["phosphorus pentoxide","1314-56-3","O10P4","Phosphoric anhydride","Phosphorus(V) oxide","Diphosphorus pentoxide","","","","",""]
["propane","74-98-6","c3h8","ch3ch2ch3","dimethyl methane","n-propane","propyl hydride","","","",""]
["propylene","115-07-1","c3h6","propene","","","","","","",""]
["n-propyl alcohol","71-23-8","CH3CH2CH2OH","1-propanol","n-propanol","Ethyl carbinol","Propyl alcohol","","","","differs in b1, b4"]
["isopropyl alcohol","67-63-0","(CH3)2CHOH","2-propanol","isopropanol","Dimethyl carbinol","IPA","sec-Propyl alcohol","Rubbing alcohol","","differs in b1, b4"]
["n-propyl benzene","103-65-1","C9H12","N-PROPYLBENZENE","1-PHENYLPROPANE","PROPYLBENZENE","N-PROPYLBENZENE","1-Propylbenzene","Isocumene;","Phenylpropane",""]
["propionic acid","79-09-4","CH3CH2COOH","Carboxyethane","Ethanecarboxylic acid","Ethylformic acid","Metacetonic acid","Methyl acetic acid","Propanoic acid","",""]
["propylene oxide","75-56-9","C3H6O","1,2-Epoxy propane","Methyl ethylene oxide","Methyloxirane","Propene oxide","1,2-Propylene oxide","","",""]
["pyridine","110-86-1","C5H5N","Azabenzene","Azine","","","","","",""]
["silicon dioxide","7631-86-9","SiO2","silica","","","","","","",""]
["sodium bicarbonate","144-55-8","CHNaO3","Sodium hydrogen carbonate","baking soda","bicarbonate of soda","nahcolite","sodium hydrogencarbonate","","",""]
["sodium bisulfate","7681-38-1","NaHSO4","Sodium hydrogen sulfate","Sodium acid sulfate","Bisulfate of soda","","","","",""]
["sodium carbonate","497-19-8","na2co3","soda ash","washing soda","soda crystals","","","","",""]
["sodium carbonate decahydrate","6132-02-1","na2co3·10h2o","na2co310h2o","","","","","","",""]
["sodium chloride","7647-14-5","NaCl","salt","table salt","common salt","halite","rock salt","saline","sodium chloric",""]
["sodium cyanide","143-33-9","NaCN","","","","","","","",""]
["sodium hydroxide","1310-73-2","NaOH","Caustic soda","Lye","Soda lye","Sodium hydrate","","","",""]
["sodium nitrate","7631-99-4","NaNO3","Caliche","Chile saltpeter","Nitrate of soda","Nitratine","Peru saltpeter","soda niter","cublic niter","saltpeter"]
["sodium nitrite","7632-00-0","NaNO2","","","","","","","",""]
["sodium sulfate","7757-82-6","Na2SO4","Thenardite","Glauber's salt","Sal mirabilis","Mirabilite","","","",""]
["sodium sulfide","1313-82-2","Na2S","Disodium sulfide","","","","","","",""]
["sodium sulfite","7757-83-7","Na2SO3","hypo clear",null,"","","","","",""]
["sodium thiosulfate","7772-98-7","Na2S2O3","Sodium hyposulfite","Hyposulphite of soda","","","","","",""]
["styrene","100-42-5","C6H5CHCH2","Ethenyl benzene","Phenylethylene","Styrol","Vinyl benzene"]
["sulfur (rhombic)","7704-34-9","S8","rhombic sulfur","sulfur rhombic","orthorhombic sulfur","flowers of sulfur","roll sulfur","milk of sulfur","α-sulfur","alpha sulfur"]
["sulfur (monoclinic)","7704-34-9","S8","monoclinic sulfur","sulfur monoclinic","prismatic sulfur","β-sulfur","beta sulfur","b-sulfur"]
["sulfuric acid","7664-93-9","H2SO4","Battery acid","Hydrogen sulfate","Oil of vitriol"]
["sulfur dioxide","7446-09-5 ","SO2","Sulfurous acid anhydride","Sulfurous oxide","Sulfur oxide"]
["sulfur trioxide","7446-11-9","SO3","Sulfuric anhydride","Sulfan","Sulfonylideneoxidane"]
["toluene","108-88-3","C6H5CH3","C7H8","Methyl benzene","Methyl benzol","Phenyl methane","Toluol"]
["1,1,1-trichlorothane","71-55-6","CH3CCl3","Chlorothene","Methyl chloroform"]
["1,1,2-trichlorothane","79-00-5","CHCl2CH2Cl","Ethane trichloride","β-Trichloroethane","Vinyl trichloride"]
["trichloroethylene","79-01-6","ClCHCCl2","Ethylene trichloride","TCE","Trichloroethene","Trilene"]
["vinyl acetate","108-05-4","CH2CHOOCCH3","1-Acetoxyethylene","Ethenyl acetate","Ethenyl ethanoate","VAC","Vinyl ethanoate"]
["water","7732-18-5","H2O","Oxidane","Hydrogen oxide","Dihydrogen monoxide","Hydrogen monoxide","Hydrogen hydroxide"]
["m-xylene","108-38-3","C6H4(CH3)2","1,3-Dimethylbenzene","meta-Xylene","m-Xylol"]
["o-xylene","95-47-6","C6H4(CH3)3","1,2-Dimethylbenzene","ortho-Xylene","o-Xylol"]
["p-xylene","106-42-3","C6H4(CH3)4","1,4-Dimethylbenzene","para-Xylene","p-Xylol"]
["zinc","7440-66-6","Zn","spelter"]

{"sheet":"B1","index":25,"n_rows":136,"n_cols":22,"rows_kept":136,"cut":false,"hidden":true,"merged":[[2,3,2,4],[2,14,2,17],[2,18,2,21]]}
["Physical Properties"]
[]
["Compound","Formula","Mol Wt","SG",null,"Tm  ","ΔĤ m (Tm )","Tb","T(decomp)","T(sublim)","T(ingite)","ΔĤ v (Tb)","Tc","Pc","ΔĤf° (kJ/mol)",null,null,null,"ΔĤc° (kJ/mol)"]
[null,null,null,"ref. Temp","value","°C","kJ/mol","°C","°C","°C","°C","kJ/mol","K","atm","(g)","(l)","(aq)","( c)","(g)","(l)","(c )","(s)"]
["Acetaldehyde","CH3CHO",44.05,18,0.78300000000000003,-123.7,null,20.2,null,null,null,25.1,461,null,-166.2,null,null,null,-1192.4000000000001]
["Acetic acid","CH3COOH",60.05,"20/4",1.0489999999999999,16.600000000000001,12.09,118.2,null,null,null,24.39,594.79999999999995,57.1,-438.15,-486.18,null,null,-919.73,-871.69]
["Acetone","C3H6O",58.08,"20/4",0.79100000000000004,-95,5.69,56,null,null,null,30.2,508,47,-216.7,-248.2,null,null,-1821.4,-1785.7]
["Acetylene","C2H2",26.04,null,null,null,null,-81.5,null,null,null,17.600000000000001,309.5,61.6,226.75,null,null,null,-1299.5999999999999]
["Ammonia","NH3",17.03,null,null,-77.8,5.6529999999999996,-33.43,null,null,null,23.350999999999999,405.5,111.3,-46.19,-67.2,null,null,-382.58]
["Ammonium hydroxide","NH4OH",35.03,null,null,null,null,null,null,null,null,null,null,null,null,null,-366.48]
["Ammonium nitrate","NH4NO3",80.05,25,1.7250000000000001,169.6,5.4,null,210,null,null,null,null,null,null,null,-399.36,-365.14]
["Ammonium sulfate","N2H8SO4",132.13999999999999,"20/4",1.7689999999999999,513,null,null,513,null,null,null,null,null,null,null,-1173.0999999999999,-1179.3]
["Aniline","C6H7N",93.12,"20/4",1.022,-6.3,null,184.2,null,null,null,null,699,52.4]
["Benzaldehyde","C6H5CHO",106.12,"20/4",1.046,-26,null,179,null,null,null,38.4,null,null,-40.04,-88.83,null,null,null,-3520]
["Benzene","C6H6",78.11,"20/4",0.879,5.53,9.8369999999999997,80.099999999999994,null,null,null,30.765000000000001,562.6,48.6,82.93,48.66,null,null,-3301.5,-3267.6]
["Benzoic acid","C7H6O2",122.12,15,1.266,122.2,null,249.8,null,null,null,null,null,null,null,null,null,null,-3226.7]
["Benzyl alcohol","C7H8O",108.13,"20/4",1.0449999999999999,-15.4,null,205.2,null,null,null,null,null,null,null,null,null,null,null,-3741.8]
["Bromine","Br2",159.83000000000001,"20/4",3.1190000000000002,-7.4,10.8,58.6,null,null,null,31,584,102,null,0]
["1,2-Butadiene","C4H6",54.09,null,null,-136.5,null,10.1,null,null,null,null,446]
["1,3-Butadiene","C4H6",54.09,null,null,-109.1,null,-4.5999999999999996,null,null,null,null,425,42.7]
["n-Butane","C4H10",58.12,null,null,-138.30000000000001,4.6609999999999996,-0.6,null,null,null,22.305,425.17,37.47,-124.7,-147,null,null,-2878.5,-2855.6]
["Isobutane","C4H10",58.12,null,null,-159.6,4.54,-11.73,null,null,null,21.292000000000002,408.1,36,-134.5,-158.4,null,null,-2868.8,-2849]
["1-Butene","C4H8",56.1,null,null,-185.3,3.8479999999999999,-6.25,null,null,null,21.916,419.6,39.700000000000003,1.17,null,null,null,-2718.6]
["Calcium carbide","CaC2",64.099999999999994,18,2.2200000000000002,2300,null,null,null,null,null,null,null,null,null,null,null,-62.76]
["Calcium carbonate","CaCO3",100.09,"20/4",2.93,null,null,null,825,null,null,null,null,null,null,null,null,-1206.9000000000001]
["Calcium chloride","CaCl2",110.99,15,2.1520000000000001,782,28.37,">1600",null,null,null,null,null,null,null,null,null,-794.96]
["Calcium hydroxide","CaO2H2",74.099999999999994,"20/4",2.2400000000000002,null,null,null,null,null,null,null,null,null,null,null,null,-986.59]
["Calcium oxide","CaO",56.08,"20/4",3.32,2570,50,2850,null,null,null,null,null,null,null,null,null,-635.6]
["Calcium phosphate","Ca3P2O8",310.19,"20/4",3.14,1670,null,null,null,null,null,null,null,null,null,null,null,-4138]
["Calcium silicate","CaSiO3",116.17,"20/4",2.915,1530,48.62,null,null,null,null,null,null,null,null,null,null,-1584]
["Calcium sulfate","CaSO4",136.15,"20/4",2.96,null,null,null,null,null,null,null,null,null,null,null,-1450.4,-1432.7]
["Calcium sulfate","CaSO4*2H2O",172.18,"20/4",2.3199999999999998,null,null,null,null,null,null,null,null,null,null,null,null,-2021]
["Carbon","C",12.01,"20/4",2.2599999999999998,3600,46,4200,null,null,null,null,null,null,null,null,null,0,null,null,-393.51]
["Carbon dioxide","CO2",44.01,null,null,-56.6,8.33,null,null,-78,null,null,304.2,72.900000000000006,-393.5,-412.9]
["Carbon disulfide","CS2",76.14,"22/20",1.2609999999999999,-112.1,4.3899999999999997,46.25,null,null,null,26.8,552,78,115.3,87.9,null,null,1102.5999999999999,-1075.2]
["Carbon monoxide","CO",28.01,null,null,-205.1,0.83699999999999997,-191.5,null,null,null,6.0419999999999998,133,34.5,-110.52,null,null,null,-282.99]
["Carbon tetrachloride","CCl4",153.84,"20/4",1.595,-22.9,2.5099999999999998,76.7,null,null,null,30,556.4,45,-106.7,-139.5,null,null,-385,-352.2]
["Chlorine","Cl2",70.91,null,null,-101,6.4059999999999997,-34.06,null,null,null,20.399999999999999,417,76.099999999999994,0]
["Chlorobenzene","C6H5Cl",112.56,"20/4",1.107,-45,null,132.1,null,null,null,36.5,632.4,44.6]
["Chloroform","CHCl3",119.39,"20/4",1.4890000000000001,-63.7,null,61,null,null,null,null,536,54,null,-131.80000000000001,null,null,null,-373]
["Copper","Cu",63.54,"20/4",8.92,1083,13.01,2595,null,null,null,304.60000000000002,null,null,null,null,null,0]
["Cupric sulfate","CuSO4",159.61000000000001,15,3.6059999999999999,null,null,null,">600",null,null,null,null,null,null,null,-843.1,-769.9]
["Cyclohexane","C6H12",84.16,"20/4",0.77900000000000003,6.7,2.677,80.7,null,null,null,30.1,553.70000000000005,40.4,-123.1,-156.19999999999999,null,null,-3953,-3919.9]
["Cyclopentane","C5H10",70.13,"20/4",0.745,-93.4,0.60899999999999999,49.3,null,null,null,27.3,511.8,44.55,-77.2,-105.9,null,null,-3319.5,-3290.9]
["n-Decane","C10H22",142.28,"20/4",0.73,-29.9,null,173.8,null,null,null,null,619,20.8,null,-249.7,null,null,-6829.7,-6778.3]
["Diethyl ether","C4H10O",74.12,25,0.70799999999999996,-116.3,7.3,34.6,null,null,null,26.05,467,35.6,null,-272.8,null,null,null,-2726.7]
["Ethane","C2H6",30.07,null,null,-183.3,2.859,-88.6,null,null,null,14.72,305.39999999999998,48.2,-84.67,null,null,null,-1559.9]
["Ethyl acetate","C4H8O2",88.1,"20/4",0.90100000000000002,-83.8,null,77,null,null,null,null,523.1,37.799999999999997,-426.8,-463.2,null,null,null,-2246.4]
["Ethyl alcohol","C2H5OH",46.07,"20/4",0.78900000000000003,-114.6,5.0209999999999999,78.5,null,null,null,38.58,516.29999999999995,63,-235.31,-277.63,null,null,-1409.25,-1366.91]
["Ethyl benzene","C8H10",106.16,"20/4",0.86699999999999999,-94.67,9.1630000000000003,136.19999999999999,null,null,null,35.979999999999997,619.70000000000005,37,29.79,-12.46,null,null,-4607.1000000000004,-4564.8999999999996]
["Ethyl bromide","C2H5Br",108.98,"20/4",1.46,-119.1,null,38.200000000000003,null,null,null,null,504,61.5,-54.4]
["Ethyl chloride","C2H5Cl",64.52,15,0.90300000000000002,-138.30000000000001,4.452,13.1,null,null,null,24.7,460.4,52,-105]
["3-Ethyl hexane","C8H18",114.22,"20/4",0.71699999999999997,null,null,118.5,null,null,null,34.270000000000003,567,26.4,-210.9,-250.5,null,null,-5509.8,-5407.1]
["Ethylene","C2H4",28.05,null,null,-169.2,3.35,-103.7,null,null,null,13.54,283.10000000000002,50.5,52.28,null,null,null,-1410.99]
["Ethylene glycol","C2H6O2",62.07,19,1.113,-13,11.23,197.2,null,null,null,56.9,null,null,-387.1,-451.5,null,null,null,-1179.5]
["Ferric oxide","Fe2O3",159.69999999999999,"20/4",5.12,null,null,null,1560,null,null,null,null,null,null,null,null,-822.2]
["Ferrous oxide","FeO",71.849999999999994,"20/4",5.7,null,null,null,null,null,null,null,null,null,null,null,null,-266.5]
["Ferrous sulfide","FeS",87.92,"20/4",4.84,1193,null,null,null,null,null,null,null,null,null,null,null,-95.1]
["Formaldehyde","H2CO",30.03,-20,0.81499999999999995,-92,null,-19.3,null,null,null,24.48,null,null,-115.9,null,null,null,-563.46]
["Formic Acid","CH2O2",46.03,"20/4",1.22,8.3000000000000007,12.68,100.5,null,null,null,22.25,null,null,-362.6,-409.2,null,null,null,-262.8]
["Glycerol","C3H8O3",92.09,50,1.26,18.2,18.3,290,null,null,null,null,null,null,null,-665.9,null,null,null,-1661.1]
["Helium","He",4,null,null,-269.7,0.02,-268.89999999999998,null,null,null,8.4000000000000005E-2,5.26,2.2599999999999998,0]
["n-Heptane","C7H16",100.2,"20/4",0.68400000000000005,-90.59,14.03,98.43,null,null,null,31.69,540.20000000000005,27,-187.8,-224.4,null,null,-4853.5,-4816.8999999999996]
["n-Hexane","C6H14",86.17,"20/4",0.65900000000000003,-95.32,13.03,68.739999999999995,null,null,null,28.85,507.9,29.9,-167.2,-198.8,null,null,-4194.8,-4163.1000000000004]
["Hydrogen","H2",2.016,null,null,-259.19,0.12,-252.76,null,null,null,0.90400000000000003,33.299999999999997,12.8,0,null,null,null,-285.83999999999997]
["Hydrogen bromide","HBr",80.92,null,null,-86,null,-67,null,null,null,null,null,null,-36.229999999999997]
["Hydrogen chloride","HCl",36.47,null,null,-114.2,1.99,-85,null,null,null,16.100000000000001,324.60000000000002,81.5,-92.31]
["Hydrogen cyanide","HCN",27.03,null,null,-14,null,26,null,null,null,null,null,null,130.54]
["Hydrogen fluoride","HF",20,null,null,-83,null,20,null,null,null,null,503.2,null,-268.60000000000002,null,-316.89999999999998]
["Hydrogen sulfide","H2S",34.08,null,null,-85.5,2.38,-60.3,null,null,null,18.670000000000002,373.6,88.9,-19.96,null,null,null,-562.59]
["Iodine","I2",253.8,"20/4",4.93,113.3,null,184.2,null,null,null,null,826,null,null,null,null,0]
["Iron","Fe",55.85,"20/4",7.7,1535,15.1,2800,null,null,null,354,null,null,null,null,null,0]
["Lead","Pb",207.21,"20/20",11.337,327.39999999999998,5.0999999999999996,1750,null,null,null,179.9,null,null,null,null,null,0]
["Lead Oxide","PbO",223.21,"20/4",9.5,886,11.7,1472,null,null,null,213,null,null,null,null,null,-219.2]
["Magnesium","Mg",24.32,"20/4",1.74,650,9.1999999999999993,1120,null,null,null,131.80000000000001,null,null,null,null,null,0]
["Magnesium chloride","MgCl2",95.23,25,2.3250000000000002,714,43.1,1418,null,null,null,136.80000000000001,null,null,null,null,null,-641.79999999999995]
["Magnesium hydroxide","MgO2H2",58.34,"20/4",2.4,null,null,null,350]
["Magnesium oxide","MgO",40.32,"20/4",3.65,2900,77.400000000000006,3600,null,null,null,null,null,null,null,null,null,-601.79999999999995]
["Mercury","Hg",200.61,"20/4",13.545999999999999,-38.869999999999997,null,-356.9,null,null,null,null,null,null,null,null,null,0]
["Methane","CH4",16.04,null,null,-182.5,0.94,-161.5,null,null,null,8.1790000000000003,190.7,45.8,-74.849999999999994,null,null,null,-890.36]
["Methyl acetate","C3H6O2",74.08,"20/4",0.93300000000000005,-98.9,null,57.1,null,null,null,null,506.7,46.3,null,-409.4,null,null,null,-1595]
["Methyl alcohol","CH3OH",32.04,"20/4",0.79200000000000004,-97.9,3.1669999999999998,64.7,null,null,null,35.270000000000003,513.20000000000005,78.5,-201.2,-238.6,null,null,-764,-726.6]
["Methyl amine","CH5N",31.06,-11,0.69899999999999995,-92.7,null,-6.9,null,null,null,null,429.9,73.599999999999994,-28,null,null,null,null,-1071.5]
["Methyl chloride","CH3Cl",50.49,null,null,-97.9,null,-24,null,null,null,null,416.1,65.8,-81.92]
["Methyl ethyl ketone","C4H8O",72.099999999999994,"20/4",0.80500000000000005,-87.1,null,78.2,null,null,null,32,null,null,null,null,null,null,null,-2436]
["Naphthalene","C10H8",128.16,"20/4",1.145,80,null,217.8,null,null,null,null,null,null,null,null,null,null,-5157]
["Nickel","Ni",58.69,"20/4",8.9,1452,null,2900,null,null,null,null,null,null,null,null,null,0]
["Nitric acid","HNO3",63.02,"20/4",1.502,-41.6,10.47,86,null,null,null,30.3,null,null,null,-173.23,-206.57]
["Nitrobenzene","C6H5O2N",123.11,"20/4",1.2030000000000001,5.5,null,210.7,null,null,null,null,null,null,null,null,null,null,null,-3092.8]
["Nitrogen","N2",28.02,null,null,-210,0.72,-195.8,null,null,null,5.577,126.2,33.5,0]
["Nitrogen dioxide","NO2",46.01,null,null,-9.3000000000000007,7.335,21.3,null,null,null,14.73,431,100,33.799999999999997]
["Nitric oxide","NO",30.01,null,null,-163.6,2.3010000000000002,-151.80000000000001,null,null,null,13.78,179.2,65,90.37]
["Nitrogen pentoxide","N2O5",108.02,18,1.63,30,null,47]
["Nitrogen tetraoxide","N2O4",92,"20/4",1.448,-9.5,null,21.1,null,null,null,null,431,99,9.3000000000000007]
["Nitrous oxide","N2O",44.02,-89,1.226,-91.1,null,-88.8,null,null,null,null,309.5,71.7,81.5]
["n-Nonane","C9H20",128.25,"20/4",0.71799999999999997,-53.8,null,150.6,null,null,null,null,595,23,null,-229,null,null,-6171,-6124.5]
["n-Octane","C8H18",114.22,"20/4",0.70299999999999996,-57,null,125.5,null,null,null,null,568.79999999999995,24.5,-208.4,-249.9,null,null,-5512.2,-5470.7]
["Oxalic acid","C2H2O4",90.04,"20/4",1.9,null,null,null,186,null,null,null,null,null,null,null,null,-826.8,null,null,null,-251.9]
["Oxygen","O2",32,null,null,-218.75,0.44400000000000001,-182.97,null,null,null,6.82,154.4,49.7,0]
["n-Pentane","C5H12",72.150000000000006,18,0.63,-129.6,8.3930000000000007,36.07,null,null,null,25.77,469.8,33.299999999999997,-146.4,-173,null,null,-3536.1,-3509.5]
["Isopentane","C5H12",72.150000000000006,19,0.62,-160.1,null,27.7,null,null,null,null,461,32.9,-152,-179.3,null,null,-3529.2,-3507.5]
["1-Pentene","C5H10",70.13,"20/4",0.64100000000000001,-165.2,4.9400000000000004,29.97,null,null,null,null,474,39.9,-20.9,null,null,null,-3375.8]
["Phenol","C6H5OH",94.11,25,1.071,42.5,11.43,181.4,null,null,null,null,692.1,60.5,-90.8,-158.1,null,null,null,null,null,-3063.5]
["Phosphoric acid","H3PO4",98,18,1.8340000000000001,42.3,10.54,null,null,null,null,null,null,null,null,null,-1278.5999999999999,-1281.0999999999999]
["Phosphorus (red)","P4",123.9,"20/4",2.2000000000000002,590,81.17,null,null,null,725,null,null,null,null,null,null,-17.600000000000001]
["Phosphorus (white)","P4",123.9,"20/4",1.82,44.2,2.5099999999999998,280,null,null,null,49.71,null,null,null,null,null,0]
["Phosphorus pentoxide","P2O5",141.94999999999999,"20/4",2.387,null,null,null,null,250,null,null,null,null,null,null,null,-1506.2]
["Propane","C3H8",44.09,null,null,-187.69,3.52,-42.07,null,null,null,18.77,369.9,42,-103.8,-119.8,null,null,-2220,-2204]
["Propylene","C3H6",42.08,null,null,-185.2,3,-47.7,null,null,null,18.420000000000002,365.1,45.4,20.41,null,null,null,-2058.4]
["n-Propyl alcohol","C3H7OH",60.09,"20/4",0.80400000000000005,-127,null,97.04,null,null,null,null,536.70000000000005,49.95,-255.2,-300.7,null,null,-2068.6,-2010.4]
["Isopropyl alcohol","C3H7OH",60.09,"20/4",0.78500000000000003,-89.7,null,82.24,null,null,null,null,508.8,53,null,-310.89999999999998,null,null,null,-1986.6]
["n-Propyl benzene","C9H12",120.19,"20/4",0.86199999999999999,-99.5,8.5399999999999991,159.19999999999999,null,null,null,38.24,638.70000000000005,31.3,7.82,-38.4,null,null,-5264.48,-5218.2]
["Silicon dioxide","SiO2",60.09,"20/4",2.25,1710,14.2,2230,null,null,null,null,null,null,null,null,null,-851]
["Sodium bicarbonate","NaHCO3",84.01,"20/4",2.2000000000000002,null,null,null,270,null,null,null,null,null,null,null,null,-945.6]
["Sodium bisulfate","NaHSO4",120.07,"20/4",2.742,null,null,null,null,null,null,null,null,null,null,null,null,-1126.3]
["Sodium carbonate","Na2CO3",105.99,"20/4",2.5329999999999999,null,null,null,854,null,null,null,null,null,null,null,null,-1130.9000000000001]
["Sodium chloride","NaCl",58.45,"20/4",2.1629999999999998,808,28.5,1465,null,null,null,170.7,null,null,null,null,null,-411]
["Sodium cyanide","NaCN",49.01,null,null,562,16.7,1497,null,null,null,155,null,null,null,null,null,-89.79]
["Sodium hydroxide","NaOH",40,"20/4",2.13,319,8.34,1390,null,null,null,null,null,null,null,null,-469.4,-426.6]
["Sodium nitrate","NaNO3",85,"20/4",2.2570000000000001,310,15.9,null,380,null,null,null,null,null,null,null,null,-466.7]
["Sodium nitrite","NaNO2",69,0,2.1680000000000001,271,null,null,320,null,null,null,null,null,null,null,null,-359.4]
["Sodium sulfate","Na2SO4",142.05000000000001,"20/4",2.698,890,24.3,null,null,null,null,null,null,null,null,null,null,-1384.5]
["Sodium sulfide","Na2S",78.05,"20/4",1.8560000000000001,950,6.7,null,null,null,null,null,null,null,null,null,null,-373.2]
["Sodium sulfite","Na2SO3",126.05,15,2.633,null,null,null,25,null,null,null,null,null,null,null,null,-1090.3]
["Sodium thiosulfate","Na2S2O3",158.11000000000001,"20/4",1.667,null,null,null,null,null,null,null,null,null,null,null,null,-1117.0999999999999]
["Sulfur (rhombic)","S8",256.52999999999997,"20/4",2.0699999999999998,113,10.039999999999999,444.6,null,null,null,83.7,null,null,null,null,null,0]
["Sulfur (monoclinic)","S8",256.52999999999997,"20/4",1.96,119,14.17,444.6,null,null,null,83.7,null,null,null,null,null,0.3]
["Sulfur dioxide","SO2",64.069999999999993,null,null,-75.48,7.4020000000000001,-10.02,null,null,null,24.91,430.7,77.8,-296.89999999999998]
["Sulfur trioxide","SO3",80.069999999999993,null,null,16.84,25.48,43.3,null,null,null,41.8,491.4,83.8,-395.18]
["Sulfuric acid","H2SO4",98.08,18,1.8340000000000001,10.35,9.8699999999999992,null,340,null,null,null,null,null,null,-811.32,-907.51]
["Toluene","C7H8",92.13,"20/4",0.86599999999999999,-94.99,6.6189999999999998,110.62,null,null,null,33.47,593.9,40.299999999999997,50,12,null,null,-3947.9,-3909.9]
["Water","H20",18.015999999999998,4,1,0,6.0095000000000001,100,null,null,null,40.655999999999999,647.4,218.3,-241.83,-285.83999999999997]
["m-Xylene","C8H10",106.16,"20/4",0.86399999999999999,-47.87,11.569000000000001,139.1,null,null,null,36.4,619,34.6,17.239999999999998,-25.42,null,null,-4594.5,-4551.8999999999996]
["o-Xylene","C8H10",106.16,"20/4",0.88,-25.18,13.598000000000001,144.41999999999999,null,null,null,36.82,631.5,35.700000000000003,18.989999999999998,-24.44,null,null,-4596.3,-4552.8999999999996]
["p-Xylene","C8H10",106.16,"20/4",0.86099999999999999,13.26,17.11,138.35,null,null,null,36.07,618,33.9,17.95,-24.43,null,null,-4595.2,-4552.91]
["Zinc","Zn",65.38,"20/4",7.14,419.5,6.6740000000000004,907,null,null,null,114.77,null,null,null,null,null,0]

{"sheet":"B2","index":26,"n_rows":73,"n_cols":12,"rows_kept":73,"cut":false,"hidden":true,"merged":[]}
["Heat Capacities"]
[]
["Compound","Formula","Mol. Wt.","State","Form","Temp. Unit","a*10^3","b*10^5","c*10^8","d*10^12","Lower limit","Upper limit"]
["Acetone","CH3COCH3",58.08,"l",1,"C",123,18.600000000000001,null,null,-30,60]
["Acetone","CH3COCH3",58.08,"g",1,"C",71.959999999999994,20.100000000000001,-12.78,34.76,0,1200]
["Acetylene","C2H2",26.04,"g",1,"C",42.43,6.0529999999999999,-5.0330000000000004,18.2,0,1200]
["Air",null,29,"g",1,"C",28.94,0.41470000000000001,0.31909999999999999,-1.9650000000000001,0,1500]
["Air",null,29,"g",1,"K",28.09,0.19650000000000001,0.47989999999999999,-1.9650000000000001,273,1800]
["Ammonia","NH3",17.03,"g",1,"C",35.15,2.9540000000000002,0.44209999999999999,-6.6859999999999999,0,1200]
["Ammonium Sulfate","N2H8SO4",132.15,"c",1,"K",215.9,null,null,null,275,328]
["Benzene","C6H6",78.11,"l",1,"C",126.5,23.4,null,null,6,67]
["Benzene","C6H6",78.11,"g",1,"C",74.06,32.950000000000003,-25.2,77.569999999999993,0,1200]
["Isobutane","C4H10",58.12,"g",1,"C",89.46,30.13,-18.91,49.87,0,1200]
["n-Butane","C4H10",58.12,"g",1,"C",92.3,27.88,-15.47,34.979999999999997,0,1200]
["Isobutene","C4H8",56.1,"g",1,"C",82.88,25.64,-17.27,50.5,0,1200]
["Calcium carbide","CaC2",64.099999999999994,"c",2,"K",68.62,1.19,{"$f":"-8.66*10^10","v":-86600000000},null,298,720]
["Calcium carbonate","CaCO3",100.09,"c",2,"K",82.34,4.9749999999999996,{"$f":"-12.87*10^10","v":-128699999999.99998},null,273,1033]
["Calcium hydroxide","CaO2H2",74.099999999999994,"c",1,"K",89.5,null,null,null,276,373]
["Calcium oxide","CaO",56.08,"c",2,"K",41.84,2.0299999999999998,{"$f":"-4.52*10^10","v":-45199999999.999992},null,273,1173]
["Carbon","C",12.01,"c",2,"K",11.18,1.095,{"$f":"-4.891*10^10","v":-48910000000},null,273,1373]
["Carbon dioxide","CO2",44.01,"g",1,"C",36.11,4.2329999999999997,-2.887,7.4640000000000004,0,1500]
["Carbon monoxide","CO",28.01,"g",1,"C",28.95,0.41099999999999998,0.3548,-2.2200000000000002,0,1500]
["Carbon tetrachloride","CCl4",153.84,"l",1,"K",93.39,12.98,null,null,273,343]
["Chlorine","Cl2",70.91,"g",1,"C",33.6,1.367,-1.607,6.4729999999999999,0,1200]
["Copper","Cu",63.54,"c",1,"K",22.76,0.61170000000000002,null,null,273,1357]
["Cumene (Isopropyl benzene)","C9H12",120.19,"g",1,"C",139.19999999999999,53.76,-39.79,120.5,0,1200]
["Cyclohexane","C6H12",84.16,"g",1,"C",94.14,49.62,-31.9,80.63,0,1200]
["Cyclopentane","C5H10",70.13,"g",1,"C",73.39,39.28,-25.54,68.66,0,1200]
["Ethane","C2H6",30.07,"g",1,"C",49.37,13.92,-5.8159999999999998,7.28,0,1200]
["Ethyl alcohol","C2H5OH",46.07,"l",1,"C",103.1,null,null,null,0]
["Ethyl alcohol","C2H5OH",46.07,"l",1,"C",158.80000000000001,null,null,null,100]
["Ethyl alcohol","C2H5OH",46.07,"g",1,"C",61.34,15.72,-8.7490000000000006,19.829999999999998,0,1200]
["Ethylene","C2H4",28.05,"g",1,"C",40.75,11.47,-6.891,17.66,0,1200]
["Ferric oxide","Fe2O3",159.69999999999999,"c",2,"K",103.4,6.7110000000000003,{"$f":"-17.72*10^10","v":-177200000000},null,273,1097]
["Formaldehyde","CH2O",30.03,"g",1,"C",34.28,4.2679999999999998,0,-8.6940000000000008,0,1200]
["Helium","He",4,"g",1,"C",20.8,null,null,null,0,1200]
["n-Hexane","C6H14",86.17,"l",1,"C",216.3,null,null,null,20,100]
["n-Hexane","C6H14",86.17,"g",1,"C",137.44,40.85,-23.92,57.66,0,1200]
["Hydrogen","H2",2.016,"g",1,"C",28.84,7.6499999999999997E-3,0.32879999999999998,-0.86980000000000002,0,1500]
["Hydrogen bromide","HBr",80.92,"g",1,"C",29.1,-2.2700000000000001E-2,0.98870000000000002,-4.8579999999999997,0,1200]
["Hydrogen chloride","HCl",36.47,"g",1,"C",29.13,-0.1341,0.97150000000000003,-4.335,0,1200]
["Hydrogen cyanide","HCN",27.03,"g",1,"C",35.299999999999997,2.9079999999999999,-1.0920000000000001,null,0,1200]
["Hydrogen sulfide","H2S",34.08,"g",1,"C",33.51,1.5469999999999999,0.30120000000000002,-3.2919999999999998,0,1500]
["Magnesium chloride","MgCl2",95.23,"c",1,"K",72.400000000000006,1.58,null,null,273,991]
["Magnesium oxide","MgO",40.32,"c",2,"K",45.44,0.50080000000000002,{"$f":"-8.732*10^10","v":-87320000000},null,273,2073]
["Methane","CH4",16.04,"g",1,"C",34.31,5.4690000000000003,0.36609999999999998,-11,0,1200]
["Methane","CH4",16.04,"g",1,"K",19.87,5.0209999999999999,1.268,-11,273,1500]
["Methyl alcohol","CH3OH",32.04,"l",1,"C",75.86,16.829999999999998,null,null,0,65]
["Methyl alcohol","CH3OH",32.04,"g",1,"C",42.93,8.3010000000000002,-1.87,-8.0299999999999994,0,700]
["Methyl cyclohexane","C7H14",98.18,"g",1,"C",121.3,56.53,-37.72,100.8,0,1200]
["Methyl cyclopentane","C6H12",84.16,"g",1,"C",98.83,45.856999999999999,-30.44,83.81,0,1200]
["Nitric acid","NHO3",63.02,"l",1,"C",110,null,null,null,25]
["Nitric oxide","NO",30.01,"g",1,"C",29.5,0.81879999999999997,-0.29249999999999998,0.36520000000000002,0,3500]
["Nitrogen","N2",28.02,"g",1,"C",29,0.21990000000000001,0.57230000000000003,-2.871,0,1500]
["Nitrogen dioxide","NO2",46.01,"g",1,"C",36.07,3.97,-2.88,7.87,0,1200]
["Nitrogen tetraoxide","N2O4",92.02,"g",1,"C",75.7,12.5,-11.3,null,0,300]
["Nitrous oxide","N2O",44.02,"g",1,"C",37.659999999999997,4.1509999999999998,-2.694,10.57,0,1200]
["Oxygen","O2",32,"g",1,"C",29.1,1.1579999999999999,-0.60760000000000003,1.3109999999999999,0,1500]
["n-Pentane","C5H12",72.150000000000006,"l",1,"C",155.4,43.68,null,null,0,36]
["n-Pentane","C5H12",72.150000000000006,"g",1,"C",114.8,34.090000000000003,-18.989999999999998,42.26,0,1200]
["Propane","C3H8",44.09,"g",1,"C",68.031999999999996,22.59,-13.11,31.71,0,1200]
["Propylene","C3H6",42.08,"g",1,"C",59.58,17.71,-10.17,24.6,0,1200]
["Sodium carbonate","Na2CO3",105.99,"c",1,"K",121,null,null,null,288,371]
["Sodium carbonate decahydrate","Na2CO3*10H2O",286.14999999999998,"c",1,"K",535.6,null,null,null,298]
["Sulfur (Rhombic)","S",32.07,"c",1,"K",15.2,2.68,null,null,273,368]
["Sulfur (Monoclinic)","S",32.07,"c",1,"K",18.3,1.84,null,null,368,392]
["Sulfuric acid","H2SO4",98.08,"l",1,"C",139.1,15.59,null,null,10,45]
["Sulfur dioxide","SO2",64.069999999999993,"g",1,"C",38.909999999999997,3.9039999999999999,-3.1040000000000001,8.6059999999999999,0,1500]
["Sulfur trioxide","SO3",80.069999999999993,"g",1,"C",48.5,9.1880000000000006,-8.5399999999999991,32.4,0,1000]
["Toluene","C7H8",92.13,"l",1,"C",148.80000000000001,32.4,null,null,0,110]
["Toluene","C7H8",92.13,"g",1,"C",94.18,38,-27.86,80.33,0,1200]
["Water","H2O",18.015999999999998,"l",1,"C",75.400000000000006,null,null,null,0,100]
["Water","H2O",18.015999999999998,"g",1,"C",33.46,0.68799999999999994,0.76039999999999996,-3.593,0,1500]

{"sheet":"Solver","index":27,"n_rows":31,"n_cols":11,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
[]
["Variables:","n1","n2","n3","n4","n5","n6","n7","n8"]
["Values:",17.696750869566571,23.090031783905591,44.584879268642737,14.631024417407591,42.748222112732797,20.567853296457333,5.000022298187802,13.992419416805889]
["8 variables require 8 equations"]
[null,"LHS","RHS","(LHS-RHS)^2"]
[1,35,{"$f":"0.673*B3+C3","v":34.999945119123893},{"$f":"(B6-C6)^2","v":3.0119105622413805E-9}]
[2,50,{"$f":"0.306*B3+D3","v":50.000085034730105},{"$f":"(B7-C7)^2","v":7.2309053240895301E-9}]
[3,15,{"$f":"0.021*B3+E3","v":15.002656185668489},7.0553223054841004E-6]
[4,{"$f":"+C3","v":23.090031783905591},{"$f":"0.059*F3+G3","v":23.089998401108566},1.1144111371771411E-9]
[5,{"$f":"+D3","v":44.584879268642737},{"$f":"0.926*F3+H3","v":44.584875974578374},1.0850860030890857E-11]
[6,{"$f":"+E3","v":14.631024417407591},{"$f":"0.015*F3+I3","v":14.633642748496881},6.8556576931390362E-6]
[7,{"$f":"+H3","v":5.000022298187802},{"$f":"0.1*50","v":5},4.9720917925202839E-10]
[8,{"$f":"+I3","v":13.992419416805889},{"$f":"0.933*15","v":13.995000000000001},6.6594096217317249E-6]
[null,null,"Sum",{"$f":"SUM(D6:D13)","v":2.058225490741765E-5}]
[]
[]
["Variables","n0","n1","n2","n3","n4","n5","n6","ntot","e1","e2"]
[null,89.730903032589111,10.809575755006403,83.063001522134911,6.1274227230593796,95.317846968107091,0.54047878775222835,10.269096967249578,195.31784696829263,83.063001522156668,6.127422723059512]
["10 variables require 10 equations"]
[null,"LHS","RHS","(LHS-RHS)^2"]
[1,{"$f":"+B18+H18","v":99.999999999838693},100,{"$f":"(B21-C21)^2","v":2.6020081124926263E-20}]
[2,{"$f":"+C18","v":10.809575755006403},{"$f":"100-J18-K18","v":10.80957575478382},4.9543121128718594E-20]
[3,{"$f":"+D18","v":83.063001522134911},{"$f":"+J18","v":83.063001522156668},4.733591542432635E-22]
[4,{"$f":"+E18","v":6.1274227230593796},{"$f":"+K18","v":6.127422723059512},1.7513500956811683E-26]
[5,{"$f":"+F18","v":95.317846968107091},{"$f":"+J18+2*K18","v":95.317846968275688},2.8425144096892745E-20]
[6,{"$f":"+I18","v":195.31784696829263},{"$f":"+C18+D18+E18+F18","v":195.31784696830778},2.2948526664021199E-22]
[7,{"$f":"+J18*(J18+2*K18)/(100-J18-K18)/(100+J18+2*K18)","v":3.7499999911530444},3.75,7.8268623610259048E-17]
[8,{"$f":"+K18*(J18+2*K18)^2/(100-J18-K18)/(100+J18+2*K18)^2","v":0.1350000050221806},0.13500000000000001,2.5222297859143884E-17]
[9,{"$f":"+G18","v":0.54047878775222835},{"$f":"0.05*C18","v":0.54047878775032021},3.6409994518947231E-24]
[10,{"$f":"+C18","v":10.809575755006403},{"$f":"+G18+H18","v":10.809575755001806},2.1134353579114402E-23]
[null,null,null,{"$f":"SUM(D21:D30)","v":1.0359563745304089E-16}]